RFC 9826 | YANG Data Model for PCEP | August 2025
Dhody, et al. | Standards Track | [Page]

Stream:
  Internet Engineering Task Force (IETF)
RFC:
  9826
Category:
  Standards Track
Published:
  August 2025
ISSN:
  2070-1721
Authors:
  D. Dhody, Ed.
  Huawei
  V. Beeram
  Juniper Networks
  J. Hardwick
  J. Tantsura
  Nvidia

# RFC 9826

# A YANG Data Model for the Path Computation Element Communication Protocol (PCEP)

## Abstract

This document defines a YANG data model for the management of the Path Computation Element Communication Protocol (PCEP) for communications between a Path Computation Client (PCC) and a Path Computation Element (PCE), or between two PCEs.¶

## Status of This Memo

This is an Internet Standards Track document.¶

This document is a product of the Internet Engineering Task Force (IETF). It represents the consensus of the IETF community. It has received public review and has been approved for publication by the Internet Engineering Steering Group (IESG). Further information on Internet Standards is available in Section 2 of RFC 7841.¶

Information about the current status of this document, any errata, and how to provide feedback on it may be obtained at https://www.rfc-editor.org/info/rfc9826.¶

## Copyright Notice

Copyright (c) 2025 IETF Trust and the persons identified as the document authors. All rights reserved.¶

This document is subject to BCP 78 and the IETF Trust's Legal Provisions Relating to IETF Documents (https://trustee.ietf.org/license-info) in effect on the date of publication of this document. Please review these documents carefully, as they describe your rights and restrictions with respect to this document. Code Components extracted from this document must include Revised BSD License text as described in Section 4.e of the Trust Legal Provisions and are provided without warranty as described in the Revised BSD License.¶

## 1. Introduction

The Path Computation Element (PCE) defined in [RFC4655] is an entity that is capable of computing a network path or route based on a network graph and applying computational constraints. A Path Computation Client (PCC) may make requests to a PCE for paths to be computed.¶

PCEP is the communication protocol between a PCC and PCE; it is defined in [RFC5440]. PCEP interactions include path computation requests and path computation replies as well as notifications of specific states related to the use of a PCE in the context of Multiprotocol Label Switching (MPLS) and Generalized MPLS (GMPLS) Traffic Engineering (TE). [RFC8231] specifies extensions to PCEP to enable stateful control of MPLS-TE Label Switched Paths (LSPs). [RFC8664] and [RFC9603] extend PCEP to support Segment Routing in MPLS and IPv6, respectively.¶

This document defines a YANG 1.1 [RFC7950] data model for the management of PCEP speakers. It is important to establish a common data model for how PCEP speakers are identified, configured, and monitored. The data model includes configuration data and state data.¶

This document contains a specification of the PCEP YANG module "ietf-pcep", which provides the PCEP [RFC5440] data model. Further, this document also includes the PCEP statistics YANG module "ietf-pcep-stats", which provides statistics, counters, and telemetry data.¶

The YANG modules in this document conform to the Network Management Datastore Architecture (NMDA) [RFC8342]. The origin of the data is indicated as per the origin metadata annotation.¶

## 2. Requirements Language

The key words "MUST", "MUST NOT", "REQUIRED", "SHALL", "SHALL NOT", "SHOULD", "SHOULD NOT", "RECOMMENDED", "NOT RECOMMENDED", "MAY", and "OPTIONAL" in this document are to be interpreted as described in BCP 14 [RFC2119] [RFC8174] when, and only when, they appear in all capitals, as shown here.¶

## 3. Terminology and Notation

This document uses the terminology defined in [RFC4655] and [RFC5440]. In particular, it uses the following:¶

- Path Computation Request (PCReq) message¶

- Path Computation Reply (PCRep) message¶

- Path Computation Notification (PCNtf) message¶

- Path Computation Error (PCErr) message¶

- Request Parameters (RP) object¶

- Synchronization Vector (SVEC) object¶

- Explicit Route Object (ERO)¶

This document uses the following terms defined in [RFC7420]:¶

PCEP entity:
  a local PCEP speaker¶
PCEP peer:
  a remote PCEP speaker¶
PCEP speaker:
  term used when it is not necessary to distinguish between local and remote.¶

Further, this document uses the following terms defined in [RFC8051]:¶

- Stateful PCE¶
- Passive Stateful PCE¶
- Active Stateful PCE¶
- Delegation¶

In addition, this document uses the following terms defined in [RFC8231]:¶

- Revocation¶
- Redelegation¶
- Path Computation LSP State Report (PCRpt) message¶
- Path Computation LSP Update Request (PCUpd) message¶
- PLSP-ID (a PCEP-specific identifier for the LSP)¶
- Stateful PCE Request Parameter (SRP)¶

This document also uses the following terms defined in [RFC8281]:¶

- PCE-initiated LSP¶

- Path Computation LSP Initiate (PCInitiate) message¶

Last, this document uses the following terms, which are defined in the RFCs indicated below:¶

- Path Setup Type (PST) [RFC8408]¶

- Segment Routing (SR) [RFC8664]¶

- Objective Function (OF) [RFC5541]¶

- Association [RFC8697]¶

- Configuration data [RFC6241]¶

- State data [RFC6241]¶

### 3.1. Tree Diagrams

Simplified graphical representations of the data model are used in this document. The meaning of the symbols in these diagrams is defined in [RFC8340].¶

### 3.2. Prefixes in Data Node Names

In this document, the names of data nodes and other data model objects are often used without a prefix, as long as it is clear from the context in which YANG module each name is defined. Otherwise, names are prefixed using the standard prefix associated with the corresponding YANG module, as shown in Table 1.¶

Table 1: Prefixes and Corresponding YANG Modules
Prefix | YANG module | Reference
--- | --- | ---
yang | ietf-yang-types | [RFC6991]
inet | ietf-inet-types | [RFC6991]
te-types | ietf-te-types | [RFC8776]
key-chain | ietf-key-chain | [RFC8177]
nacm | ietf-netconf-acm | [RFC8341]
tlss | ietf-tls-server | [RFC9645]
tlsc | ietf-tls-client | [RFC9645]
ospf | ietf-ospf | [RFC9129]
isis | ietf-isis | [RFC9130]

### 3.3. References in the YANG Data Model

The following table lists the documents that are referenced in the YANG data model defined in this document.¶

Table 2: References in the YANG Data Model
Documents | Reference
--- | ---
OSPF Protocol Extensions for Path Computation Element (PCE) Discovery | [RFC5088]
IS-IS Protocol Extensions for Path Computation Element (PCE) Discovery | [RFC5089]
Path Computation Element (PCE) Communication Protocol (PCEP) | [RFC5440]
Preserving Topology Confidentiality in Inter-Domain Path Computation Using a Path-Key-Based Mechanism | [RFC5520]
Encoding of Objective Functions in the Path Computation Element Communication Protocol (PCEP) | [RFC5541]
Path Computation Element Communication Protocol (PCEP) Requirements and Protocol Extensions in Support of Global Concurrent Optimization | [RFC5557]
Common YANG Data Types | [RFC6991]
YANG Data Model for Key Chains | [RFC8177]
Path Computation Element Communication Protocol (PCEP) Extensions for Stateful PCE | [RFC8231]
Optimizations of Label Switched Path State Synchronization Procedures for a Stateful PCE | [RFC8232]
PCEPS: Usage of TLS to Provide a Secure Transport for the Path Computation Element Communication Protocol (PCEP) | [RFC8253]
Path Computation Element Communication Protocol (PCEP) Extensions for PCE-Initiated LSP Setup in a Stateful PCE Model | [RFC8281]
Extensions to the Path Computation Element Communication Protocol (PCEP) for Point-to-Multipoint Traffic Engineering Label Switched Paths | [RFC8306]
Network Configuration Access Control Model | [RFC8341]
Conveying Path Setup Type in PCE Communication Protocol (PCEP) Messages | [RFC8408]
Common YANG Data Types for Traffic Engineering | [RFC8776]
YANG Groupings for TLS Clients and TLS Servers | [RFC9645]
Path Computation Element Communication Protocol (PCEP) Extensions for Segment Routing | [RFC8664]
Path Computation Element Communication Protocol (PCEP) Extensions for Establishing Relationships between Sets of Label Switched Paths (LSPs) | [RFC8697]
YANG Data Model for the OSPF Protocol | [RFC9129]
YANG Data Model for the IS-IS Protocol | [RFC9130]
Path Computation Element Communication Protocol (PCEP) Extensions for GMPLS | [RFC8779]
"ASSOCIATION Type Field" registry (in the "Path Computation Element Protocol (PCEP) Numbers" registry group) | [IANA-PCEP]
"Path Computation Element (PCE) Capability Flags" registry (in the "Interior Gateway Protocol (IGP) Parameters" registry group) | [IANA-IGP]
Path Computation Element Communication Protocol (PCEP) Extension for Flow Specification | [RFC9168]
Path Computation Element Communication Protocol (PCEP) Extensions for the Hierarchical Path Computation Element (H-PCE) Architecture | [RFC8685]
Hierarchical Stateful Path Computation Element (PCE) | [RFC8751]
IGP Extension for Path Computation Element Communication Protocol (PCEP) Security Capability Support in PCE Discovery (PCED) | [RFC9353]
Stateful Path Computation Element (PCE) Protocol Extensions for Usage with Point-to-Multipoint TE Label Switched Paths (LSPs) | [RFC8623]
The TCP Authentication Option | [RFC5925]
Path Computation Element Communication Protocol (PCEP) Extensions for Associating Working and Protection Label Switched Paths (LSPs) with Stateful PCE | [RFC8745]
Path Computation Element Communication Protocol (PCEP) Extension for Label Switched Path (LSP) Diversity Constraint Signaling | [RFC8800]
Path Computation Element Communication Protocol (PCEP) Extensions for Establishing Relationships between Sets of Label Switched Paths and Virtual Networks | [RFC9358]
Extensions to the Path Computation Element Communication Protocol (PCEP) for Inter-Layer MPLS and GMPLS Traffic Engineering | [RFC8282]
Path Computation Element Communication Protocol (PCEP) Extension for Associating Policies and Label Switched Paths (LSPs) | [RFC9005]

## 4. The Design of PCEP Data Model

The PCEP YANG module defined in this document has all the common building blocks for PCEP, which are listed below and further detailed in the subsequent subsections.¶

- The local PCEP entity¶

- The PCEP peer¶

- The PCEP session¶

- Notifications¶

- RPC¶

    module: ietf-pcep
      +--rw pcep!
         +--rw entity
            +--rw addr*                         inet:ip-address-no-zone
            +--rw enabled?                      boolean
            +--rw role                          role
            +--rw description?                  string
            +--rw speaker-entity-id?            string {sync-opt}?
            +--rw admin-status?                 boolean
            +--ro index?                        uint32
            +--ro oper-status?                  oper-status
            +--rw domains
            |  +--rw domain* [type domain]
            |     +--...
            +--rw capabilities
            |  +--...
            +--rw auth
            |  +--...
            +--rw pce-info
            |  +--rw scope
            |  |  +--...
            |  +--rw neighbor-domains
            |  |  +--...
            |  +--rw path-key {path-key}?
            |     +--...
            +--...
            +--ro lsp-db {stateful}?
            |  +--ro db-ver?             uint64 {sync-opt}?
            |  +--ro association-list*
            |  |       [type id source global-source extended-id]
            |  |       {association}?
            |  |  +--...
            |  +--ro lsp* [plsp-id pcc-id lsp-id]
            |     +--...
            +--ro path-keys {path-key}?
            |  +--ro path-key* [key]
            |     +--...
            +--rw peers
               +--rw peer* [addr]
                  +--...
                  +--ro sessions
                     +--ro session* [initiator]
                        +--...

      rpcs:
        +---x trigger-resync {stateful,sync-opt}?
           +---w input
              +---w pcc    -> /pcep/entity/peers/peer/addr

      notifications:
        +---n pcep-session-up
        |  +--...
        +---n pcep-session-down
        |  +--...
        +---n pcep-session-local-overload
        |  +--...
        +---n pcep-session-local-overload-clear
        |  +--...
        +---n pcep-session-peer-overload
        |  +--...
        +---n pcep-session-peer-overload-clear
           +--...

¶

### 4.1. The Entity

The PCEP YANG module may contain status information for the local PCEP entity.¶

The entity has an IP address (using ietf-inet-types [RFC6991]) and a "role" leaf (the local entity PCEP role) as mandatory.¶

Note that the PCEP MIB module [RFC7420] uses an entity list and a system-generated entity index as a primary index to the read-only entity table.¶

The local PCEP entity contains various information related to this entity such as its domain, capabilities, security parameters, etc. When the local entity is PCE, it could also have path-key and the LSP Database (LSP-DB) information.¶

Note that the timer names in YANG use hyphens as compared to [RFC5440] (for example, DeadTimer in the protocol specification is called dead-timer in YANG).¶

    module: ietf-pcep
      +--rw pcep!
         +--rw entity
            +--rw addr*                         inet:ip-address-no-zone
            +--rw enabled?                      boolean
            +--rw role                          role
            +--rw description?                  string
            +--rw speaker-entity-id?            string {sync-opt}?
            +--rw admin-status?                 boolean
            +--ro index?                        uint32
            +--ro oper-status?                  oper-status
            +--rw domains
            |  +--rw domain* [type domain]
            |     +--rw type      identityref
            |     +--rw domain    domain
            +--rw capabilities
            |  +--rw capability?             bits
            |  +--rw pce-initiated?          boolean {pce-initiated}?
            |  +--rw include-db-ver?         boolean {stateful,sync-opt}?
            |  +--rw trigger-resync?         boolean {stateful,sync-opt}?
            |  +--rw trigger-initial-sync?   boolean {stateful,sync-opt}?
            |  +--rw incremental-sync?       boolean {stateful,sync-opt}?
            |  +--rw sr-mpls {sr-mpls}?
            |  |  +--rw enabled?        boolean
            |  |  +--rw no-msd-limit?   boolean
            |  |  +--rw nai?            boolean
            |  +--rw stateful-gmpls {stateful,gmpls}?
            |  |  +--rw enabled?   boolean
            |  +--rw inter-layer?            boolean {inter-layer}?
            |  +--rw h-pce {h-pce}?
            |     +--rw enabled?    boolean
            |     +--rw stateful?   boolean {stateful}?
            |     +--rw role?       hpce-role
            +--ro msd?                          uint8 {sr-mpls}?
            +--rw auth
            |  +--rw (auth-type-selection)?
            |     +--:(auth-key-chain)
            |     |  +--rw key-chain?
            |     |          key-chain:key-chain-ref
            |     +--:(auth-key)
            |     |  +--rw crypto-algorithm            identityref
            |     |  +--rw (key-string-style)?
            |     |     +--:(keystring)
            |     |     |  +--rw keystring?            string
            |     |     +--:(hexadecimal) {key-chain:hex-key-string}?
            |     |        +--rw hexadecimal-string?   yang:hex-string
            |     +--:(auth-tls) {tls}?
            |        +--rw (role)?
            |           +--:(server)
            |           |  +--rw tls-server
            |           |     +--rw server-identity
            |           |     |  +--rw (auth-type)
            |           |     |        ...
            |           |     +--rw client-authentication!
            |           |     |       {client-auth-supported}?
            |           |     |  +--rw ca-certs! {client-auth-x509-cert}?
            |           |     |  |     ...
            |           |     |  +--rw ee-certs! {client-auth-x509-cert}?
            |           |     |  |     ...
            |           |     |  +--rw raw-public-keys!
            |           |     |  |       {client-auth-raw-public-key}?
            |           |     |  |     ...
            |           |     |  +--rw tls12-psks?        empty
            |           |     |  |       {client-auth-tls12-psk}?
            |           |     |  +--rw tls13-epsks?       empty
            |           |     |          {client-auth-tls13-epsk}?
            |           |     +--rw hello-params {tlscmn:hello-params}?
            |           |     |  +--rw tls-versions
            |           |     |  |     ...
            |           |     |  +--rw cipher-suites
            |           |     |        ...
            |           |     +--rw keepalives {tls-server-keepalives}?
            |           |        +--rw peer-allowed-to-send?   empty
            |           |        +--rw test-peer-aliveness!
            |           |              ...
            |           +--:(client)
            |              +--rw tls-client
            |                 +--rw client-identity!
            |                 |  +--rw (auth-type)
            |                 |        ...
            |                 +--rw server-authentication
            |                 |  +--rw ca-certs! {server-auth-x509-cert}?
            |                 |  |     ...
            |                 |  +--rw ee-certs! {server-auth-x509-cert}?
            |                 |  |     ...
            |                 |  +--rw raw-public-keys!
            |                 |  |       {server-auth-raw-public-key}?
            |                 |  |     ...
            |                 |  +--rw tls12-psks?        empty
            |                 |  |       {server-auth-tls12-psk}?
            |                 |  +--rw tls13-epsks?       empty
            |                 |          {server-auth-tls13-epsk}?
            |                 +--rw hello-params {tlscmn:hello-params}?
            |                 |  +--rw tls-versions
            |                 |  |     ...
            |                 |  +--rw cipher-suites
            |                 |        ...
            |                 +--rw keepalives {tls-client-keepalives}?
            |                    +--rw peer-allowed-to-send?   empty
            |                    +--rw test-peer-aliveness!
            |                          ...
            +--rw pce-info
            |  +--rw scope
            |  |  +--rw path-scope?         bits
            |  |  +--rw intra-area-pref?    uint8
            |  |  +--rw inter-area-pref?    uint8
            |  |  +--rw inter-as-pref?      uint8
            |  |  +--rw inter-layer-pref?   uint8
            |  +--rw neighbor-domains
            |  |  +--rw domain* [type domain]
            |  |     +--rw type      identityref
            |  |     +--rw domain    domain
            |  +--rw path-key {path-key}?
            |     +--rw enabled?         boolean
            |     +--rw discard-timer?   uint32
            |     +--rw reuse-time?      uint32
            |     +--rw pce-id?          inet:ip-address-no-zone
            +--rw connect-timer?                uint16
            +--rw connect-max-retry?            uint32
            +--rw init-back-off-timer           uint16
            +--rw max-back-off-timer            uint32
            +--ro open-wait-timer?              uint16
            +--ro keep-wait-timer?              uint16
            +--rw keepalive-timer?              uint8
            +--rw dead-timer?                   uint8
            +--rw allow-negotiation?            boolean
            +--rw max-keepalive-timer           uint8
            +--rw max-dead-timer                uint8
            +--rw min-keepalive-timer           uint8
            +--rw min-dead-timer                uint8
            +--rw sync-timer?                   uint16 {svec}?
            +--rw request-timer                 uint16
            +--rw max-sessions                  uint32
            +--rw max-unknown-reqs?             uint32
            +--rw max-unknown-msgs?             uint32
            +--rw pcep-notification-max-rate    uint32
            +--rw stateful-parameter {stateful}?
            |  +--rw state-timeout           uint32
            |  +--rw redelegation-timeout    uint32
            |  +--rw rpt-non-pcep-lsp?       boolean
            +--rw of-list {objective-function}?
            |  +--rw objective-function* [of]
            |     +--rw of    identityref
            +--ro lsp-db {stateful}?
            |  +--ro db-ver?             uint64 {sync-opt}?
            |  +--ro association-list*
            |  |       [type id source global-source extended-id]
            |  |       {association}?
            |  |  +--ro type             identityref
            |  |  +--ro id               uint16
            |  |  +--ro source           inet:ip-address-no-zone
            |  |  +--ro global-source    uint32
            |  |  +--ro extended-id      string
            |  |  +--ro lsp* [plsp-id pcc-id lsp-id]
            |  |     +--ro plsp-id    -> /pcep/entity/lsp-db/lsp/plsp-id
            |  |     +--ro pcc-id     leafref
            |  |     +--ro lsp-id     leafref
            |  +--ro lsp* [plsp-id pcc-id lsp-id]
            |     +--ro plsp-id               uint32
            |     +--ro pcc-id                inet:ip-address-no-zone
            |     +--ro source?               inet:ip-address-no-zone
            |     +--ro destination?          inet:ip-address-no-zone
            |     +--ro tunnel-id?            uint16
            |     +--ro lsp-id                uint16
            |     +--ro extended-tunnel-id?   inet:ip-address-no-zone
            |     +--ro admin-state?          boolean
            |     +--ro operational-state?    operational-state
            |     +--ro delegated
            |     |  +--ro enabled?   boolean
            |     |  +--ro peer?      -> /pcep/entity/peers/peer/addr
            |     |  +--ro srp-id?    uint32
            |     +--ro initiation {pce-initiated}?
            |     |  +--ro enabled?   boolean
            |     |  +--ro peer?      -> /pcep/entity/peers/peer/addr
            |     +--ro symbolic-path-name?   string
            |     +--ro last-error?           identityref
            |     +--ro pst?                  identityref
            |     +--ro association-list*
            |             [type id source global-source extended-id]
            |             {association}?
            |        +--ro type
            |        |       -> /pcep/entity/lsp-db/association-list/type
            |        +--ro id               leafref
            |        +--ro source           leafref
            |        +--ro global-source    leafref
            |        +--ro extended-id      leafref
            +--ro path-keys {path-key}?
            |  +--ro path-key* [key]
            |     +--ro key              uint16
            |     +--ro cps
            |     |  +--ro explicit-route-objects* [index]
            |     |     +--ro index    uint32
            |     |     +--ro (type)?
            |     |        +--:(numbered-node-hop)
            |     |        |  +--ro numbered-node-hop
            |     |        |     +--ro node-id     te-node-id
            |     |        |     +--ro hop-type?   te-hop-type
            |     |        +--:(numbered-link-hop)
            |     |        |  +--ro numbered-link-hop
            |     |        |     +--ro link-tp-id    te-tp-id
            |     |        |     +--ro hop-type?     te-hop-type
            |     |        |     +--ro direction?    te-link-direction
            |     |        +--:(unnumbered-link-hop)
            |     |        |  +--ro unnumbered-link-hop
            |     |        |     +--ro link-tp-id    te-tp-id
            |     |        |     +--ro node-id       te-node-id
            |     |        |     +--ro hop-type?     te-hop-type
            |     |        |     +--ro direction?    te-link-direction
            |     |        +--:(as-number)
            |     |        |  +--ro as-number-hop
            |     |        |     +--ro as-number    inet:as-number
            |     |        |     +--ro hop-type?    te-hop-type
            |     |        +--:(label)
            |     |           +--ro label-hop
            |     |              +--ro te-label
            |     |                    ...
            |     +--ro pcc-requester?   -> /pcep/entity/peers/peer/addr
            |     +--ro req-id?          uint32
            |     +--ro retrieved?       boolean
            |     +--ro pcc-retrieved?   -> /pcep/entity/peers/peer/addr
            |     +--ro creation-time?   yang:timestamp
            |     +--ro discard-time?    uint32
            |     +--ro reuse-time?      uint32
            +--rw peers
               +--rw peer* [addr]
                  +--...

¶

#### 4.1.1. The Peer List

The peer list contains peer(s) that the local PCEP entity knows about. A PCEP speaker is identified by its IP address. If there is a PCEP speaker in the network that uses multiple IP addresses, then it looks like multiple distinct peers to the other PCEP speakers in the network.¶

Since PCEP sessions can be ephemeral, the peer list tracks a peer even when no PCEP session currently exists for that peer. The statistics contained are an aggregate of the statistics for all successive sessions with that peer.¶

To limit the quantity of information that is stored, an implementation MAY choose to discard this information if and only if no PCEP session exists for the corresponding peer.¶

The data model for PCEP peers presented in this document uses a flat list of peers. Each peer in the list is identified by its IP address.¶

This peer list includes peers that are explicitly configured at the local PCEP entity as well as peers that are learned dynamically. For example, at a PCC, the remote PCE peer to use could be explicitly configured. A PCC could also learn a PCE address in the network via the IGP discovery, and it will show up in this list. When a session is initiated at a PCE, the remote PCC peer information is also added by the system to the peer list.¶

    module: ietf-pcep
      +--rw pcep!
         +--rw entity
            +--...
            +--rw peers
               +--rw peer* [addr]
                  +--rw addr                    inet:ip-address-no-zone
                  +--rw role                    role
                  +--rw description?            string
                  +--rw domains
                  |  +--rw domain* [type domain]
                  |     +--rw type      identityref
                  |     +--rw domain    domain
                  +--rw capabilities
                  |  +--rw capability?             bits
                  |  +--rw pce-initiated?          boolean
                  |  |       {pce-initiated}?
                  |  +--rw include-db-ver?         boolean
                  |  |       {stateful,sync-opt}?
                  |  +--rw trigger-resync?         boolean
                  |  |       {stateful,sync-opt}?
                  |  +--rw trigger-initial-sync?   boolean
                  |  |       {stateful,sync-opt}?
                  |  +--rw incremental-sync?       boolean
                  |  |       {stateful,sync-opt}?
                  |  +--rw sr-mpls {sr-mpls}?
                  |  |  +--rw enabled?        boolean
                  |  |  +--rw no-msd-limit?   boolean
                  |  |  +--rw nai?            boolean
                  |  +--rw stateful-gmpls {stateful,gmpls}?
                  |  |  +--rw enabled?   boolean
                  |  +--rw inter-layer?            boolean {inter-layer}?
                  |  +--rw h-pce {h-pce}?
                  |     +--rw enabled?    boolean
                  |     +--rw stateful?   boolean {stateful}?
                  |     +--rw role?       hpce-role
                  +--ro msd?                    uint8 {sr-mpls}?
                  +--rw pce-info
                  |  +--rw scope
                  |  |  +--rw path-scope?         bits
                  |  |  +--rw intra-area-pref?    uint8
                  |  |  +--rw inter-area-pref?    uint8
                  |  |  +--rw inter-as-pref?      uint8
                  |  |  +--rw inter-layer-pref?   uint8
                  |  +--rw neighbor-domains
                  |     +--rw domain* [type domain]
                  |        +--rw type      identityref
                  |        +--rw domain    domain
                  +--rw delegation-pref         uint8 {stateful}?
                  +--rw auth
                  |  +--rw (auth-type-selection)?
                  |     +--:(auth-key-chain)
                  |     |  +--rw key-chain?
                  |     |          key-chain:key-chain-ref
                  |     +--:(auth-key)
                  |     |  +--rw crypto-algorithm            identityref
                  |     |  +--rw (key-string-style)?
                  |     |     +--:(keystring)
                  |     |     |  +--rw keystring?            string
                  |     |     +--:(hexadecimal)
                  |     |              {key-chain:hex-key-string}?
                  |     |        +--rw hexadecimal-string?
                  |     |                yang:hex-string
                  |     +--:(auth-tls) {tls}?
                  |        +--rw (role)?
                  |           +--:(server)
                  |           |  +--rw tls-server
                  |           |        ...
                  |           +--:(client)
                  |              +--rw tls-client
                  |                    ...
                  +--ro discontinuity-time?     yang:timestamp
                  +--ro initiate-session?       boolean
                  +--ro session-exists?         boolean
                  +--ro session-up-time?        yang:timestamp
                  +--ro session-fail-time?      yang:timestamp
                  +--ro session-fail-up-time?   yang:timestamp
                  +--ro sessions
                     +--ro session* [initiator]
                        +--...

¶

##### 4.1.1.1. The Session List

The session list contains PCEP sessions that the PCEP entity (PCE or PCC) is currently participating in. The statistics in session are semantically different from those in peer since the former applies to the current session only, whereas the latter is the aggregate for all sessions that have existed to that peer.¶

Although [RFC5440] forbids more than one active PCEP session between a given pair of PCEP entities at any given time, there is a window during the session establishment where two sessions may exist for a given pair, one representing a session initiated by the local PCEP entity and the other representing a session initiated by the peer. When one of these sessions reaches the active state, then the other is discarded.¶

The data model for the PCEP session presented in this document uses a flat list of sessions. Each session in the list is identified by its initiator. This index allows two sessions to exist transiently for a given peer, as discussed above.¶

    module: ietf-pcep
      +--rw pcep!
         +--rw entity
            +--...
            +--rw peers
               +--rw peer* [addr]
                  +--...
                  +--ro sessions
                     +--ro session* [initiator]
                        +--ro initiator                    initiator
                        +--ro role?
                        |       -> ../../../role
                        +--ro state-last-change?           yang:timestamp
                        +--ro state?                       sess-state
                        +--ro session-creation?            yang:timestamp
                        +--ro connect-retry?               yang:counter32
                        +--ro local-id?                    uint8
                        +--ro remote-id?                   uint8
                        +--ro keepalive-timer?             uint8
                        +--ro peer-keepalive-timer?        uint8
                        +--ro dead-timer?                  uint8
                        +--ro peer-dead-timer?             uint8
                        +--ro ka-hold-time-rem?            uint8
                        +--ro overloaded?                  boolean
                        +--ro overloaded-timestamp?        yang:timestamp
                        +--ro overload-time?               uint32
                        +--ro peer-overloaded?             boolean
                        +--ro peer-overloaded-timestamp?   yang:timestamp
                        +--ro peer-overload-time?          uint32
                        +--ro lspdb-sync?                  sync-state
                        |       {stateful}?
                        +--ro recv-db-ver?                 uint64
                        |       {stateful,sync-opt}?
                        +--ro of-list {objective-function}?
                        |  +--ro objective-function* [of]
                        |     +--ro of    identityref
                        +--ro pst-list
                        |  +--ro path-setup-type* [pst]
                        |     +--ro pst    identityref
                        +--ro assoc-type-list {association}?
                        |  +--ro assoc-type* [at]
                        |     +--ro at    identityref
                        +--ro speaker-entity-id?           string
                                {sync-opt}?

¶

### 4.2. Notifications

This YANG data model defines a list of notifications to inform clients of important events detected during the protocol operation. The notifications defined cover the PCEP MIB [RFC7420] notifications.¶

      notifications:
        +---n pcep-session-up
        |  +--ro peer-addr?           -> /pcep/entity/peers/peer/addr
        |  +--ro session-initiator?   leafref
        |  +--ro state-last-change?   yang:timestamp
        |  +--ro state?               sess-state
        +---n pcep-session-down
        |  +--ro peer-addr?           -> /pcep/entity/peers/peer/addr
        |  +--ro session-initiator?   initiator
        |  +--ro state-last-change?   yang:timestamp
        |  +--ro state?               sess-state
        +---n pcep-session-local-overload
        |  +--ro peer-addr?              -> /pcep/entity/peers/peer/addr
        |  +--ro session-initiator?      leafref
        |  +--ro overloaded?             boolean
        |  +--ro overloaded-timestamp?   yang:timestamp
        |  +--ro overload-time?          uint32
        +---n pcep-session-local-overload-clear
        |  +--ro peer-addr?
        |  |       -> /pcep/entity/peers/peer/addr
        |  +--ro overloaded?                   boolean
        |  +--ro overloaded-clear-timestamp?   yang:timestamp
        +---n pcep-session-peer-overload
        |  +--ro peer-addr?
        |  |       -> /pcep/entity/peers/peer/addr
        |  +--ro session-initiator?           leafref
        |  +--ro peer-overloaded?             boolean
        |  +--ro peer-overloaded-timestamp?   yang:timestamp
        |  +--ro peer-overload-time?          uint32
        +---n pcep-session-peer-overload-clear
           +--ro peer-addr?
           |       -> /pcep/entity/peers/peer/addr
           +--ro peer-overloaded?                   boolean
           +--ro peer-overloaded-clear-timestamp?   yang:timestamp

¶

### 4.3. RPC

This YANG data model defines an RPC to trigger state resynchronization at the PCE for a sanity check with a particular PCC.¶

      rpcs:
        +---x trigger-resync {stateful,sync-opt}?
           +---w input
              +---w pcc    -> /pcep/entity/peers/peer/addr

¶

## 5. The Design of PCEP Statistics Data Model

The "ietf-pcep-stats" module augments the "ietf-pcep" module to include statistics at the PCEP peer and session level. It also includes an RPC to reset all PCEP statistics across all peers and sessions through mechanisms such as walking a list of pointers to those peer and session statistics.¶

If this mechanism is not supported, implementations must reset PCEP statistics by invoking the action 'reset-statistics' for each peer and session.¶

    module: ietf-pcep-stats

      augment /pcep:pcep/pcep:entity/pcep:peers/pcep:peer:
        +--ro stats
           +--ro discontinuity-time?   yang:timestamp
           +--ro pce
           |  +--ro rsp-time-avg?           uint32
           |  +--ro rsp-time-lwm?           uint32
           |  +--ro rsp-time-hwm?           uint32
           |  +--ro pcreq-sent?             yang:counter32
           |  +--ro pcreq-rcvd?             yang:counter32
           |  +--ro pcrep-sent?             yang:counter32
           |  +--ro pcrep-rcvd?             yang:counter32
           |  +--ro req-sent?               yang:counter32
           |  +--ro req-sent-pend-rep?      yang:counter32
           |  +--ro req-sent-ero-rcvd?      yang:counter32
           |  +--ro req-sent-nopath-rcvd?   yang:counter32
           |  +--ro req-sent-cancel-rcvd?   yang:counter32
           |  +--ro req-sent-error-rcvd?    yang:counter32
           |  +--ro req-sent-timeout?       yang:counter32
           |  +--ro req-sent-cancel-sent?   yang:counter32
           |  +--ro rep-rcvd-unknown?       yang:counter32
           +--ro pcerr-sent?           yang:counter32
           +--ro pcerr-rcvd?           yang:counter32
           +--ro pcntf-sent?           yang:counter32
           +--ro pcntf-rcvd?           yang:counter32
           +--ro keepalive-sent?       yang:counter32
           +--ro keepalive-rcvd?       yang:counter32
           +--ro unknown-rcvd?         yang:counter32
           +--ro corrupt-rcvd?         yang:counter32
           +--ro pcc
           |  +--ro req-rcvd?               yang:counter32
           |  +--ro req-rcvd-pend-rep?      yang:counter32
           |  +--ro req-rcvd-ero-sent?      yang:counter32
           |  +--ro req-rcvd-nopath-sent?   yang:counter32
           |  +--ro req-rcvd-cancel-sent?   yang:counter32
           |  +--ro req-rcvd-error-sent?    yang:counter32
           |  +--ro req-rcvd-cancel-rcvd?   yang:counter32
           |  +--ro req-rcvd-unknown?       yang:counter32
           +--ro svec {pcep:svec}?
           |  +--ro pce
           |  |  +--ro svec-sent?       yang:counter32
           |  |  +--ro svec-req-sent?   yang:counter32
           |  +--ro pcc
           |     +--ro svec-rcvd?       yang:counter32
           |     +--ro svec-req-rcvd?   yang:counter32
           +--ro stateful {pcep:stateful}?
           |  +--ro pce
           |  |  +--ro pcrpt-sent?             yang:counter32
           |  |  +--ro pcupd-rcvd?             yang:counter32
           |  |  +--ro rpt-sent?               yang:counter32
           |  |  +--ro upd-rcvd?               yang:counter32
           |  |  +--ro upd-rcvd-unknown?       yang:counter32
           |  |  +--ro upd-rcvd-undelegated?   yang:counter32
           |  |  +--ro upd-rcvd-error-sent?    yang:counter32
           |  +--ro pcc
           |  |  +--ro pcrpt-rcvd?            yang:counter32
           |  |  +--ro pcupd-sent?            yang:counter32
           |  |  +--ro rpt-rcvd?              yang:counter32
           |  |  +--ro rpt-rcvd-error-sent?   yang:counter32
           |  |  +--ro upd-sent?              yang:counter32
           |  +--ro initiation {pcep:pce-initiated}?
           |     +--ro pcc
           |     |  +--ro pcinitiate-sent?   yang:counter32
           |     |  +--ro initiate-sent?     yang:counter32
           |     +--ro pce
           |        +--ro pcinitiate-rcvd?            yang:counter32
           |        +--ro initiate-rcvd?              yang:counter32
           |        +--ro initiate-rcvd-error-sent?   yang:counter32
           +--ro path-key {pcep:path-key}?
           |  +--ro unknown-path-key?      yang:counter32
           |  +--ro exp-path-key?          yang:counter32
           |  +--ro dup-path-key?          yang:counter32
           |  +--ro path-key-no-attempt?   yang:counter32
           +---x reset-statistics
           |  +---w input
           |  |  +---w reset-at?   yang:date-and-time
           |  +--ro output
           |     +--ro reset-finished-at?   yang:date-and-time
           +--ro sess-setup-ok?        yang:counter32
           +--ro sess-setup-fail?      yang:counter32
           +--ro req-sent-closed?      yang:counter32
           +--ro req-rcvd-closed?      yang:counter32
      augment /pcep:pcep/pcep:entity/pcep:peers/pcep:peer/pcep:sessions
                /pcep:session:
        +--ro stats
           +--ro discontinuity-time?   yang:timestamp
           +--ro pce
           |  +--ro rsp-time-avg?           uint32
           |  +--ro rsp-time-lwm?           uint32
           |  +--ro rsp-time-hwm?           uint32
           |  +--ro pcreq-sent?             yang:counter32
           |  +--ro pcreq-rcvd?             yang:counter32
           |  +--ro pcrep-sent?             yang:counter32
           |  +--ro pcrep-rcvd?             yang:counter32
           |  +--ro req-sent?               yang:counter32
           |  +--ro req-sent-pend-rep?      yang:counter32
           |  +--ro req-sent-ero-rcvd?      yang:counter32
           |  +--ro req-sent-nopath-rcvd?   yang:counter32
           |  +--ro req-sent-cancel-rcvd?   yang:counter32
           |  +--ro req-sent-error-rcvd?    yang:counter32
           |  +--ro req-sent-timeout?       yang:counter32
           |  +--ro req-sent-cancel-sent?   yang:counter32
           |  +--ro rep-rcvd-unknown?       yang:counter32
           +--ro pcerr-sent?           yang:counter32
           +--ro pcerr-rcvd?           yang:counter32
           +--ro pcntf-sent?           yang:counter32
           +--ro pcntf-rcvd?           yang:counter32
           +--ro keepalive-sent?       yang:counter32
           +--ro keepalive-rcvd?       yang:counter32
           +--ro unknown-rcvd?         yang:counter32
           +--ro corrupt-rcvd?         yang:counter32
           +--ro pcc
           |  +--ro req-rcvd?               yang:counter32
           |  +--ro req-rcvd-pend-rep?      yang:counter32
           |  +--ro req-rcvd-ero-sent?      yang:counter32
           |  +--ro req-rcvd-nopath-sent?   yang:counter32
           |  +--ro req-rcvd-cancel-sent?   yang:counter32
           |  +--ro req-rcvd-error-sent?    yang:counter32
           |  +--ro req-rcvd-cancel-rcvd?   yang:counter32
           |  +--ro req-rcvd-unknown?       yang:counter32
           +--ro svec {pcep:svec}?
           |  +--ro pce
           |  |  +--ro svec-sent?       yang:counter32
           |  |  +--ro svec-req-sent?   yang:counter32
           |  +--ro pcc
           |     +--ro svec-rcvd?       yang:counter32
           |     +--ro svec-req-rcvd?   yang:counter32
           +--ro stateful {pcep:stateful}?
           |  +--ro pce
           |  |  +--ro pcrpt-sent?             yang:counter32
           |  |  +--ro pcupd-rcvd?             yang:counter32
           |  |  +--ro rpt-sent?               yang:counter32
           |  |  +--ro upd-rcvd?               yang:counter32
           |  |  +--ro upd-rcvd-unknown?       yang:counter32
           |  |  +--ro upd-rcvd-undelegated?   yang:counter32
           |  |  +--ro upd-rcvd-error-sent?    yang:counter32
           |  +--ro pcc
           |  |  +--ro pcrpt-rcvd?            yang:counter32
           |  |  +--ro pcupd-sent?            yang:counter32
           |  |  +--ro rpt-rcvd?              yang:counter32
           |  |  +--ro rpt-rcvd-error-sent?   yang:counter32
           |  |  +--ro upd-sent?              yang:counter32
           |  +--ro initiation {pcep:pce-initiated}?
           |     +--ro pcc
           |     |  +--ro pcinitiate-sent?   yang:counter32
           |     |  +--ro initiate-sent?     yang:counter32
           |     +--ro pce
           |        +--ro pcinitiate-rcvd?            yang:counter32
           |        +--ro initiate-rcvd?              yang:counter32
           |        +--ro initiate-rcvd-error-sent?   yang:counter32
           +--ro path-key {pcep:path-key}?
           |  +--ro unknown-path-key?      yang:counter32
           |  +--ro exp-path-key?          yang:counter32
           |  +--ro dup-path-key?          yang:counter32
           |  +--ro path-key-no-attempt?   yang:counter32
           +---x reset-statistics
              +---w input
              |  +---w reset-at?   yang:date-and-time
              +--ro output
                 +--ro reset-finished-at?   yang:date-and-time

      rpcs:
        +---x reset-pcep-statistics-all {reset-all}?

¶

## 6. Advanced PCE Features

This document contains a specification of the base PCEP YANG module, "ietf-pcep", which provides the basic PCEP [RFC5440] data model.¶

This document further handles advanced PCE features such as:¶

- Capability and scope¶

- Domain information (local/neighbor)¶

- Path-key¶

- Objective Function (OF)¶

- Global Concurrent Optimization (GCO)¶

- Point-to-Multipoint (P2MP)¶

- GMPLS¶

- Inter-layer¶

- Stateful PCE¶

- Segment Routing (SR) for the MPLS data plane¶

- Authentication including PCEPS (TLS)¶

- Hierarchical PCE (H-PCE)¶

Segment Routing in the IPv6 data plane is out of the scope of this document. Refer to [YANG-PCEP-SRV6] for the PCEP-SRv6 YANG module.¶

### 6.1. Stateful PCE's LSP-DB

In the operational datastore of stateful PCE, the list of LSP state is maintained in the LSP-DB. The key is the PLSP-ID, the PCC's IP address, and the LSP-ID.¶

The PCEP data model contains the operational state of LSPs (/pcep/entity/lsp-db/lsp/) with PCEP-specific attributes. The generic TE attributes of the LSP are defined in [YANG-TE]. A reference to the LSP state in the TE model is maintained.¶

## 7. Other Considerations

### 7.1. PCEP over TLS (PCEPS)

[RFC8253] describes the use of TLS 1.2 [RFC5246] or later in PCEP. Further, [PCEPS-UPDATE] specifies how to protect PCEP messages with TLS 1.3 [RFC8446] by disallowing the use of early data (0-RTT) and listing the cipher suites that need to be supported with TLS 1.3.¶

The PCC acting as the TLS client opens the TLS connection, and the PCE acting as the TLS server listens for incoming connections as per the TLS specifications ([RFC8446] and [RFC5246]). [RFC8253] specifies the StartTLS procedure in PCEP that initiates the TLS connection before exchanging PCEP messages; thus, the identity verification is completed before the PCEP session is established.¶

Note that a PCEP speaker could act as both a client (PCC) and a server (PCE). The role within the context of a PCEP session is determined by the relationship it has with its peer (the same is true for TLS as well).¶

The YANG module uses the TLS grouping in [RFC9645]. Note that any TLS version can be configured, but [RFC9645] recommends the use of TLS 1.3 only. At the time of publication of this document, TLS 1.2 is still in common use for PCEP and can still be enabled with the feature "tls12" even though it is marked with status as "deprecated".¶

## 8. PCEP YANG Modules

### 8.1. ietf-pcep Module

    <CODE BEGINS> file "ietf-pcep@2025-09-12.yang"

    module ietf-pcep {
      yang-version 1.1;
      namespace "urn:ietf:params:xml:ns:yang:ietf-pcep";
      prefix pcep;

      import ietf-inet-types {
        prefix inet;
        reference
          "RFC 6991: Common YANG Data Types";
      }
      import ietf-yang-types {
        prefix yang;
        reference
          "RFC 6991: Common YANG Data Types";
      }
      import ietf-te-types {
        prefix te-types;
        reference
          "RFC 8776: Common YANG Data Types for Traffic Engineering";
      }
      import ietf-key-chain {
        prefix key-chain;
        reference
          "RFC 8177: YANG Data Model for Key Chains";
      }
      import ietf-netconf-acm {
        prefix nacm;
        reference
          "RFC 8341: Network Configuration Access Control Model";
      }
      import ietf-tls-server {
        prefix tlss;
        reference
          "RFC 9645: YANG Groupings for TLS Clients and TLS Servers";
      }
      import ietf-tls-client {
        prefix tlsc;
        reference
          "RFC 9645: YANG Groupings for TLS Clients and TLS Servers";
      }
      import ietf-ospf {
        prefix ospf;
        reference
          "RFC 9129: YANG Data Model for the OSPF Protocol";
      }
      import ietf-isis {
        prefix isis;
        reference
          "RFC 9130: YANG Data Model for the IS-IS Protocol";
      }

      organization
        "IETF PCE (Path Computation Element) Working Group";
      contact
        "WG Web:  <https://datatracker.ietf.org/wg/pce/>
         WG List:  <mailto:pce@ietf.org>
         Editor:   Dhruv Dhody
                  <mailto:dhruv.ietf@gmail.com>";
      description
        "The YANG module defines a generic configuration and
         operational model for the Path Computation Element
         Communication Protocol (PCEP).

         The key words 'MUST', 'MUST NOT', 'REQUIRED', 'SHALL', 'SHALL
         NOT', 'SHOULD', 'SHOULD NOT', 'RECOMMENDED', 'NOT RECOMMENDED',
         'MAY', and 'OPTIONAL' in this document are to be interpreted as
         described in BCP 14 (RFC 2119) (RFC 8174) when, and only when,
         they appear in all capitals, as shown here.

         Copyright (c) 2025 IETF Trust and the persons identified as
         authors of the code.  All rights reserved.

         Redistribution and use in source and binary forms, with or
         without modification, is permitted pursuant to, and subject to
         the license terms contained in, the Revised BSD License set
         forth in Section 4.c of the IETF Trust's Legal Provisions
         Relating to IETF Documents
         (https://trustee.ietf.org/license-info).

         This version of this YANG module is part of RFC 9826; see the
         RFC itself for full legal notices.";

      revision 2025-09-12 {
        description
          "Initial revision.";
        reference
          "RFC 9826: A YANG Data Model for the Path Computation
           Element Communication Protocol (PCEP)";
      }

      /*
       * Typedefs
       */

      typedef role {
        type enumeration {
          enum unknown {
            value 0;
            description
              "An unknown role.";
          }
          enum pcc {
            value 1;
            description
              "The role of a Path Computation Client (PCC).";
          }
          enum pce {
            value 2;
            description
              "The role of a Path Computation Element (PCE).";
          }
          enum pcc-and-pce {
            value 3;
            description
              "The role of both Path Computation Client (PCC) and
               Path Computation Element (PCE).";
          }
        }
        description
          "The role of a PCEP speaker.
           Takes one of the following values:
           - unknown(0): the role is not known,
           - pcc(1): the role is of a Path Computation
            Client (PCC),
           - pce(2): the role is of a Path Computation
            Element (PCE),
           - pcc-and-pce(3): the role is of both a PCC and
            a PCE.";
        reference
          "RFC 5440: Path Computation Element (PCE) Communication
           Protocol (PCEP)";
      }

      typedef oper-status {
        type enumeration {
          enum oper-status-up {
            value 1;
            description
              "The PCEP entity is active.";
          }
          enum oper-status-down {
            value 2;
            description
              "The PCEP entity is inactive.";
          }
          enum oper-status-going-up {
            value 3;
            description
              "The PCEP entity is activating.";
          }
          enum oper-status-going-down {
            value 4;
            description
              "The PCEP entity is deactivating.";
          }
          enum oper-status-failed {
            value 5;
            description
              "The PCEP entity has failed and will recover
               when possible.";
          }
          enum oper-status-failed-perm {
            value 6;
            description
              "The PCEP entity has failed and will not recover
               without operator intervention.";
          }
        }
        description
          "The operational status of the PCEP entity.
           Takes one of the following values:
           - oper-status-up(1): Active,
           - oper-status-down(2): Inactive,
           - oper-status-going-up(3): Activating,
           - oper-status-going-down(4): Deactivating,
           - oper-status-failed(5): Failed,
           - oper-status-failed-perm(6): Failed Permanently.";
        reference
          "RFC 5440: Path Computation Element (PCE) Communication
           Protocol (PCEP)";
      }

      typedef initiator {
        type enumeration {
          enum local {
            value 1;
            description
              "The local PCEP entity initiated the session.";
          }
          enum remote {
            value 2;
            description
              "The remote PCEP peer initiated the session.";
          }
        }
        description
          "The initiator of the session, that is, whether the TCP
           connection was initiated by the local PCEP entity or
           the remote peer.
           Takes one of the following values:
           - local(1): Initiated locally,
           - remote(2): Initiated remotely.";
      }

      typedef sess-state {
        type enumeration {
          enum tcp-pending {
            value 1;
            description
              "The TCPPending state of PCEP session.";
          }
          enum open-wait {
            value 2;
            description
              "The OpenWait state of PCEP session.";
          }
          enum keep-wait {
            value 3;
            description
              "The KeepWait state of PCEP session.";
          }
          enum session-up {
            value 4;
            description
              "The SessionUP state of PCEP session.";
          }
        }
        description
          "The current state of the session.
           The set of possible states excludes the idle state
           since entries do not exist in the idle state.
           Takes one of the following values:
           - tcp-pending(1): PCEP TCPPending state,
           - open-wait(2): PCEP OpenWait state,
           - keep-wait(3): PCEP KeepWait state,
           - session-up(4): PCEP SessionUP state.";
        reference
          "RFC 5440: Path Computation Element (PCE) Communication
           Protocol (PCEP)";
      }

      typedef domain {
        type union {
          type ospf:area-id-type;
          type isis:area-address;
          type inet:as-number;
        }
        description
          "The domain information.";
      }

      typedef operational-state {
        type enumeration {
          enum down {
            value 0;
            description
              "Not active.";
          }
          enum up {
            value 1;
            description
              "Signaled.";
          }
          enum active {
            value 2;
            description
              "Up and carrying traffic.";
          }
          enum going-down {
            value 3;
            description
              "LSP is being torn down; resources are
               being released.";
          }
          enum going-up {
            value 4;
            description
              "LSP is being signaled.";
          }
        }
        description
          "The operational status of the LSP.";
        reference
          "RFC 8231: Path Computation Element Communication Protocol
           (PCEP) Extensions for Stateful PCE";
      }

      typedef sync-state {
        type enumeration {
          enum pending {
            value 0;
            description
              "The state synchronization
               has not started.";
          }
          enum ongoing {
            value 1;
            description
              "The state synchronization
               is ongoing.";
          }
          enum finished {
            value 2;
            description
              "The state synchronization
               is finished.";
          }
        }
        description
          "The LSP-DB state synchronization operational
           status.";
        reference
          "RFC 8231: Path Computation Element Communication Protocol
           (PCEP) Extensions for Stateful PCE";
      }

      typedef hpce-role {
        type enumeration {
          enum unknown {
            value 0;
            description
              "An unknown role.";
          }
          enum child {
            value 1;
            description
              "The PCE is acting as child PCE.";
          }
          enum parent {
            value 2;
            description
              "The PCE is acting as parent PCE.";
          }
        }
        description
          "The H-PCE role of the PCE.";
        reference
          "RFC 8685: Path Computation Element Communication Protocol
           (PCEP) Extensions for the Hierarchical Path Computation
           Element (H-PCE) Architecture";
      }

      /*
       * Features
       */

      feature svec {
        description
          "Support synchronized path computation.";
        reference
          "RFC 5440: Path Computation Element (PCE) Communication
           Protocol (PCEP)";
      }

      feature gmpls {
        description
          "Support GMPLS.";
        reference
          "RFC 8779: Path Computation Element Communication Protocol
           (PCEP) Extensions for GMPLS";
      }

      feature objective-function {
        description
          "Support OF as per RFC 5541.";
        reference
          "RFC 5541: Encoding of Objective Functions in the Path
           Computation Element Communication Protocol (PCEP)";
      }

      feature global-concurrent {
        description
          "Support Global Concurrent Optimization (GCO) as per RFC
           5557.";
        reference
          "RFC 5557: Path Computation Element Communication Protocol
           (PCEP) Requirements and Protocol Extensions in Support of
           Global Concurrent Optimization";
      }

      feature path-key {
        description
          "Support path-key as per RFC 5520.";
        reference
          "RFC 5520: Preserving Topology Confidentiality in Inter-
           Domain Path Computation Using a Path-Key-Based Mechanism";
      }

      feature p2mp {
        description
          "Support Point-to-Multipoint (P2MP) as per RFC 8306.";
        reference
          "RFC 8306: Extensions to the Path Computation Element
           Communication Protocol (PCEP) for Point-to-Multipoint
           Traffic Engineering Label Switched Paths";
      }

      feature stateful {
        description
          "Support stateful PCE as per RFC 8231.";
        reference
          "RFC 8231: Path Computation Element Communication Protocol
           (PCEP) Extensions for Stateful PCE";
      }

      feature sync-opt {
        description
          "Support stateful state synchronization optimization
           as per RFC 8232.";
        reference
          "RFC 8232: Optimizations of Label Switched Path State
           Synchronization Procedures for a Stateful PCE";
      }

      feature pce-initiated {
        description
          "Support PCE-initiated LSP as per
           RFC 8281.";
        reference
          "RFC 8281: Path Computation Element Communication Protocol
           (PCEP) Extensions for PCE-Initiated LSP Setup in a Stateful
           PCE Model";
      }

      feature tls {
        description
          "Support PCEP over TLS as per RFC 8253.";
        reference
          "RFC 8253: PCEPS: Usage of TLS to Provide a Secure Transport
           for the Path Computation Element Communication Protocol
           (PCEP)";
      }

      feature sr-mpls {
        description
          "Support Segment Routing (SR) for MPLS in PCEP.";
        reference
          "RFC 8664: Path Computation Element Communication Protocol
           (PCEP) Extensions for Segment Routing";
      }

      feature association {
        description
          "Support Association in PCEP.";
        reference
          "RFC 8697: Path Computation Element Communication Protocol
           (PCEP) Extensions for Establishing Relationships between
           Sets of Label Switched Paths (LSPs)";
      }

      feature flowspec {
        description
          "Support Flow Specification in PCEP.";
        reference
          "RFC 9168: Path Computation Element Communication Protocol
           (PCEP) Extension for Flow Specification";
      }

      feature h-pce {
        description
          "Support Hierarchical PCE (H-PCE).";
        reference
          "RFC 8685: Path Computation Element Communication
           Protocol (PCEP) Extensions for the Hierarchical Path
           Computation Element (H-PCE) Architecture";
      }

      feature inter-layer {
        description
          "Support inter-layer path computation.";
        reference
          "RFC 8282: Extensions to the Path Computation
           Element Communication Protocol (PCEP) for Inter-
           Layer MPLS and GMPLS Traffic Engineering";
      }

      /*
       * Identities
       */

      identity domain-type {
        description
          "Base domain type for PCE.";
      }

      identity ospf-area {
        base domain-type;
        description
          "The OSPF area.";
      }

      identity isis-area {
        base domain-type;
        description
          "The IS-IS area.";
      }

      identity autonomous-system {
        base domain-type;
        description
          "The Autonomous System (AS).";
      }

      identity lsp-error {
        if-feature "stateful";
        description
          "Base LSP error.";
        reference
          "RFC 8231: Path Computation Element Communication Protocol
           (PCEP) Extensions for Stateful PCE";
      }

      identity no-error-lsp-error {
        if-feature "stateful";
        base lsp-error;
        description
          "No error; LSP is fine.";
        reference
          "RFC 8231: Path Computation Element Communication Protocol
           (PCEP) Extensions for Stateful PCE";
      }

      identity unknown-lsp-error {
        if-feature "stateful";
        base lsp-error;
        description
          "Unknown reason.  LSP Error Code value = 1.";
        reference
          "RFC 8231: Path Computation Element Communication Protocol
           (PCEP) Extensions for Stateful PCE";
      }

      identity limit-lsp-error {
        if-feature "stateful";
        base lsp-error;
        description
          "Limit reached for PCE-controlled LSPs.  LSP Error Code
           value = 2.";
        reference
          "RFC 8231: Path Computation Element Communication Protocol
           (PCEP) Extensions for Stateful PCE";
      }

      identity pending-lsp-error {
        if-feature "stateful";
        base lsp-error;
        description
          "Too many pending LSP update requests.  LSP Error Code
           value = 3.";
        reference
          "RFC 8231: Path Computation Element Communication Protocol
           (PCEP) Extensions for Stateful PCE";
      }

      identity unacceptable-lsp-error {
        if-feature "stateful";
        base lsp-error;
        description
          "Unacceptable parameters.  LSP Error Code value = 4.";
        reference
          "RFC 8231: Path Computation Element Communication Protocol
           (PCEP) Extensions for Stateful PCE";
      }

      identity internal-lsp-error {
        if-feature "stateful";
        base lsp-error;
        description
          "Internal error.  LSP Error Code value = 5.";
        reference
          "RFC 8231: Path Computation Element Communication Protocol
           (PCEP) Extensions for Stateful PCE";
      }

      identity admin-lsp-error {
        if-feature "stateful";
        base lsp-error;
        description
          "LSP administratively brought down.  LSP Error Code value
           = 6.";
        reference
          "RFC 8231: Path Computation Element Communication Protocol
           (PCEP) Extensions for Stateful PCE";
      }

      identity preempted-lsp-error {
        if-feature "stateful";
        base lsp-error;
        description
          "LSP preempted.  LSP Error Code value = 7.";
        reference
          "RFC 8231: Path Computation Element Communication Protocol
           (PCEP) Extensions for Stateful PCE";
      }

      identity rsvp-lsp-error {
        if-feature "stateful";
        base lsp-error;
        description
          "RSVP signaling error.  LSP Error Code value = 8.";
        reference
          "RFC 8231: Path Computation Element Communication Protocol
           (PCEP) Extensions for Stateful PCE";
      }

      identity path-protection {
        base te-types:association-type;
        description
          "Path Protection Association.";
        reference
          "RFC 8745: Path Computation Element Communication Protocol
           (PCEP) Extensions for Associating Working and Protection
           Label Switched Paths (LSPs) with Stateful PCE";
      }

      identity disjoint {
        base te-types:association-type;
        description
          "Disjoint Association.";
        reference
          "RFC 8800: Path Computation Element Communication Protocol
           (PCEP) Extension for Label Switched Path (LSP) Diversity
           Constraint Signaling";
      }

      identity policy {
        base te-types:association-type;
        description
          "Policy Association.";
        reference
          "RFC 9005: Path Computation Element Communication Protocol
           (PCEP) Extension for Associating Policies and Label Switched
           Paths (LSPs)";
      }

      identity virtual-network {
        base te-types:association-type;
        description
          "Virtual Network (VN) Association.";
        reference
          "RFC 9358: Path Computation Element Communication Protocol
           (PCEP) Extensions for Establishing Relationships between
           Sets of Label Switched Paths and Virtual Networks";
      }

      /*
       * Groupings
       */

      grouping domain {
        description
          "This grouping specifies a domain where the
           PCEP speaker has topology visibility.";
        leaf type {
          type identityref {
            base domain-type;
          }
          description
            "The domain type.";
        }
        leaf domain {
          type domain;
          description
            "The domain information.";
        }
      }

      grouping domain-info {
        description
          "This grouping specifies all information that
           may be relevant to both PCC and PCE.
           This information corresponds to PCE auto-discovery
           information.
           The scope relates to either a local entity or a peer.";
        container domains {
          description
            "The domain for the local PCEP entity or a peer.";
          list domain {
            key "type domain";
            description
              "The domain information.";
            uses domain {
              description
                "The domain for the local PCEP entity or a peer.";
            }
          }
        }
        container capabilities {
          description
            "The PCEP entity or peer capability information.
             This may be relevant to PCE selection as well.
             This information corresponds to PCE auto-
             discovery information.";
          reference
            "IANA IGP: Path Computation Element (PCE) Capability
             Flags in Interior Gateway Protocol (IGP) Parameters
             RFC 5088: OSPF Protocol Extensions for Path
             Computation Element (PCE) Discovery
             RFC 5089: IS-IS Protocol Extensions for Path
             Computation Element (PCE) Discovery
             RFC 9353: IGP Extension for Path Computation Element
             Communication Protocol (PCEP) Security Capability
             Support in PCE Discovery (PCED)";
          leaf capability {
            type bits {
              bit gmpls {
                if-feature "gmpls";
                description
                  "Path computation with GMPLS link
                   constraints.";
              }
              bit bi-dir {
                description
                  "Bidirectional path computation.";
              }
              bit diverse {
                description
                  "Diverse path computation.";
              }
              bit load-balance {
                description
                  "Load-balanced path computation.";
              }
              bit synchronize {
                if-feature "svec";
                description
                  "Synchronized paths computation.";
              }
              bit objective-function {
                if-feature "objective-function";
                description
                  "Support for multiple objective functions.";
              }
              bit add-path-constraint {
                description
                  "Support for additive path constraints (max
                   hop count, etc.).";
              }
              bit prioritization {
                description
                  "Support for request prioritization.";
              }
              bit multi-request {
                description
                  "Support for multiple requests per message.";
              }
              bit global-concurrent {
                if-feature "global-concurrent";
                description
                  "Support for Global Concurrent Optimization
                   (GCO).";
                reference
                  "RFC 5557: Path Computation Element Communication
                   Protocol (PCEP) Requirements and Protocol
                   Extensions in Support of Global Concurrent
                   Optimization";
              }
              bit p2mp {
                if-feature "p2mp";
                description
                  "Support for P2MP path computation.";
                reference
                  "RFC 8306: Extensions to the Path Computation
                   Element Communication Protocol (PCEP) for
                   Point-to-Multipoint Traffic Engineering Label
                   Switched Paths";
              }
              bit active {
                if-feature "stateful";
                description
                  "Support for active stateful PCE.";
                reference
                  "RFC 8231: Path Computation Element
                   Communication Protocol (PCEP) Extensions
                   for Stateful PCE";
              }
              bit passive {
                if-feature "stateful";
                description
                  "Support for passive stateful PCE.";
                reference
                  "RFC 8231: Path Computation Element
                   Communication Protocol (PCEP) Extensions
                   for Stateful PCE";
              }
              bit p2mp-active {
                if-feature "stateful";
                if-feature "p2mp";
                description
                  "Support for active stateful PCE for P2MP.";
                reference
                  "RFC 8623: Stateful Path Computation Element
                   (PCE) Protocol Extensions for Usage with
                   Point-to-Multipoint TE Label Switched Paths
                   (LSPs)";
              }
              bit p2mp-passive {
                if-feature "stateful";
                if-feature "p2mp";
                description
                  "Support for passive stateful PCE for P2MP.";
                reference
                  "RFC 8623: Stateful Path Computation Element
                   (PCE) Protocol Extensions for Usage with
                   Point-to-Multipoint TE Label Switched Paths
                   (LSPs)";
              }
              bit p2mp-pce-initiated {
                if-feature "stateful";
                if-feature "pce-initiated";
                if-feature "p2mp";
                description
                  "Support for PCE-initiated LSP for P2MP.";
                reference
                  "RFC 8623: Stateful Path Computation Element
                   (PCE) Protocol Extensions for Usage with
                   Point-to-Multipoint TE Label Switched Paths
                   (LSPs)";
              }
              bit flowspec {
                if-feature "flowspec";
                description
                  "Support for Flow Specification.";
                reference
                  "RFC 9168: Path Computation Element Communication
                   Protocol (PCEP) Extension for Flow Specification";
              }
              bit tcp-ao {
                description
                  "Support for the TCP Authentication Option
                   (TCP-AO).";
                reference
                  "RFC 5440: Path Computation Element (PCE)
                   Communication Protocol (PCEP)
                   RFC 5925: The TCP Authentication Option";
              }
              bit tls {
                if-feature "tls";
                description
                  "Support for TLS.";
                reference
                  "RFC 8253: PCEPS: Usage of TLS to Provide a
                   Secure Transport for the Path Computation
                   Element Communication Protocol (PCEP)";
              }
            }
            description
              "The bits string indicating the capabilities.";
            reference
              "IANA IGP: Path Computation Element (PCE) Capability
               Flags in Interior Gateway Protocol (IGP) Parameters
               RFC 5088: OSPF Protocol Extensions for Path
               Computation Element (PCE) Discovery
               RFC 5089: IS-IS Protocol Extensions for Path
               Computation Element (PCE) Discovery
               RFC 9353: IGP Extension for Path Computation Element
               Communication Protocol (PCEP) Security Capability
               Support in PCE Discovery (PCED)";
          }
          leaf pce-initiated {
            if-feature "pce-initiated";
            type boolean;
            default "false";
            description
              "Set to true if PCE-initiated LSP capability is
               enabled.";
            reference
              "RFC 8281: Path Computation Element Communication
               Protocol (PCEP) Extensions for PCE-Initiated LSP
               Setup in a Stateful PCE Model";
          }
          leaf include-db-ver {
            if-feature "stateful";
            if-feature "sync-opt";
            type boolean;
            default "true";
            description
              "Support inclusion of LSP-DB-VERSION
               in LSP object.";
            reference
              "RFC 8232: Optimizations of Label Switched Path State
               Synchronization Procedures for a Stateful PCE";
          }
          leaf trigger-resync {
            if-feature "stateful";
            if-feature "sync-opt";
            type boolean;
            default "true";
            description
              "Support PCE-triggered resynchronization.";
            reference
              "RFC 8232: Optimizations of Label Switched Path State
               Synchronization Procedures for a Stateful PCE";
          }
          leaf trigger-initial-sync {
            if-feature "stateful";
            if-feature "sync-opt";
            type boolean;
            default "true";
            description
              "PCE-triggered initial synchronization.";
            reference
              "RFC 8232: Optimizations of Label Switched Path State
               Synchronization Procedures for a Stateful PCE";
          }
          leaf incremental-sync {
            if-feature "stateful";
            if-feature "sync-opt";
            type boolean;
            default "true";
            description
              "Support incremental (delta) synchronization.";
            reference
              "RFC 8232: Optimizations of Label Switched Path State
               Synchronization Procedures for a Stateful PCE";
          }
          container sr-mpls {
            if-feature "sr-mpls";
            description
              "If segment routing for MPLS is supported at the local
               entity or a peer.";
            reference
              "RFC 8664: Path Computation Element Communication Protocol
               (PCEP) Extensions for Segment Routing";
            leaf enabled {
              type boolean;
              default "false";
              description
                "Set to true if SR-MPLS is enabled.";
            }
            leaf no-msd-limit {
              type boolean;
              default "false";
              description
                "True indicates no limit on Maximum SID Depth (MSD); the
                 leaf msd is ignored.";
            }
            leaf nai {
              type boolean;
              default "false";
              description
                "True indicates the capability to resolve Node or
                 Adjacency Identifier (NAI) to Segment
                 Identifier (SID).";
            }
          }
          container stateful-gmpls {
            if-feature "stateful";
            if-feature "gmpls";
            description
              "If stateful GMPLS is supported for a local entity
               or a peer.";
            reference
              "RFC 8779: Path Computation Element Communication Protocol
               (PCEP) Extensions for GMPLS";
            leaf enabled {
              type boolean;
              default "false";
              description
                "Set to true if stateful GMPLS is enabled.";
            }
          }
          leaf inter-layer {
            if-feature "inter-layer";
            type boolean;
            default "false";
            description
              "If inter-layer path computation is supported for
               local entity or a peer.";
            reference
              "RFC 8282: Extensions to the Path Computation
               Element Communication Protocol (PCEP) for Inter-
               Layer MPLS and GMPLS Traffic Engineering";
          }
          container h-pce {
            if-feature "h-pce";
            description
              "If Hierarchical PCE (H-PCE) is supported for local
               entity or a peer.";
            reference
              "RFC 8685: Path Computation Element Communication
               Protocol (PCEP) Extensions for the Hierarchical Path
               Computation Element (H-PCE) Architecture";
            leaf enabled {
              type boolean;
              default "false";
              description
                "Set to true if H-PCE is enabled.";
            }
            leaf stateful {
              if-feature "stateful";
              type boolean;
              default "false";
              description
                "Set to true if stateful H-PCE is enabled.";
              reference
                "RFC 8751: Hierarchical Stateful Path Computation
                 Element (PCE)";
            }
            leaf role {
              when "../../../role = 'pce'"
                 + "or "
                 + "../../../role = 'pcc-and-pce'" {
                description
                  "These fields are applicable when the role is PCE.";
              }
              type hpce-role;
              description
                "The H-PCE role of the PCE.";
            }
          }
        }
        leaf msd {
          if-feature "sr-mpls";
          type uint8;
          config false;
          description
            "Maximum SID Depth (MSD) for SR-MPLS (i.e., the label stack
             depth that a PCC is capable of imposing on a packet).";
          reference
            "RFC 8664: Path Computation Element Communication Protocol
             (PCEP) Extensions for Segment Routing";
        }
      }

      grouping pce-info {
        description
          "This grouping specifies all PCE information
           that may be relevant to the PCE selection.
           This information corresponds to PCE auto-discovery
           information.";
        container scope {
          description
            "This container defines PCE path computation scope
             information that may be relevant to PCE selection.
             This information corresponds to PCE auto-discovery
             information.";
          leaf path-scope {
            type bits {
              bit intra-area-scope {
                description
                  "PCE can compute intra-area paths (L bit).";
              }
              bit inter-area-scope {
                description
                  "PCE can compute inter-area paths (R bit).";
              }
              bit inter-area-scope-default {
                description
                  "PCE can act as a default PCE for inter-area
                   path computation (Rd bit).";
              }
              bit inter-as-scope {
                description
                  "PCE can compute inter-AS paths (S bit).";
              }
              bit inter-as-scope-default {
                description
                  "PCE can act as a default PCE for inter-AS
                   path computation (Sd bit).";
              }
              bit inter-layer-scope {
                description
                  "PCE can compute inter-layer paths (Y bit).";
              }
            }
            description
              "The field corresponding to the path scope bits.";
          }
          leaf intra-area-pref {
            type uint8 {
              range "0..7";
            }
            description
              "The PCE's preference for intra-area TE LSP
               computation (PrefL field), where 7 reflects
               the highest preference.";
          }
          leaf inter-area-pref {
            type uint8 {
              range "0..7";
            }
            description
              "The PCE's preference for inter-area TE LSP
               computation (PrefR field), where 7 reflects
               the highest preference.";
          }
          leaf inter-as-pref {
            type uint8 {
              range "0..7";
            }
            description
              "The PCE's preference for inter-AS TE LSP
               computation (PrefS field), where 7 reflects
               the highest preference.";
          }
          leaf inter-layer-pref {
            type uint8 {
              range "0..7";
            }
            description
              "The PCE's preference for inter-layer TE LSP
               computation (PrefY field), where 7 reflects
               the highest preference.";
          }
          reference
            "RFC 5088: OSPF Protocol Extensions for Path
             Computation Element (PCE) Discovery
             RFC 5089: IS-IS Protocol Extensions for Path
             Computation Element (PCE) Discovery";
        }
        container neighbor-domains {
          description
            "The list of neighbor PCE domains
             toward which a PCE can compute
             paths.";
          list domain {
            key "type domain";
            description
              "The neighbor domain.";
            uses domain {
              description
                "The PCE neighbor domain.";
            }
          }
        }
      }

      grouping notification-instance-hdr {
        description
          "This group describes common instance-specific data
           for notifications.";
        leaf peer-addr {
          type leafref {
            path "/pcep/entity/peers/peer/addr";
          }
          description
            "Reference to peer address.";
        }
      }

      grouping notification-session-hdr {
        description
          "This group describes common session instance-specific
           data for notifications.";
        uses notification-instance-hdr;
        leaf session-initiator {
          type leafref {
            path "/pcep/entity/peers/peer[addr=current()/../peer-addr]/"
               + "sessions/session/initiator";
          }
          description
            "Reference to pcep session initiator leaf.";
        }
      }

      grouping of-list {
        description
          "List of Objective Functions (OF).";
        reference
          "RFC 5541: Encoding of Objective Functions in the Path
           Computation Element Communication Protocol (PCEP)";
        list objective-function {
          key "of";
          description
            "The list of authorized OF.";
          leaf of {
            type identityref {
              base te-types:objective-function-type;
            }
            description
              "The OF authorized.";
          }
        }
      }

      grouping auth {
        description
          "The authentication options.";
        container auth {
          description
            "The authentication options.";
          choice auth-type-selection {
            description
              "Options for expressing authentication
               setting.";
            case auth-key-chain {
              leaf key-chain {
                type key-chain:key-chain-ref;
                description
                  "Key-chain name.";
              }
            }
            case auth-key {
              leaf crypto-algorithm {
                type identityref {
                  base key-chain:crypto-algorithm;
                }
                mandatory true;
                description
                  "Cryptographic algorithm associated
                   with key.";
              }
              choice key-string-style {
                description
                  "Key string styles.";
                case keystring {
                  leaf keystring {
                    nacm:default-deny-all;
                    type string;
                    description
                      "Key string in ASCII format.";
                  }
                }
                case hexadecimal {
                  if-feature "key-chain:hex-key-string";
                  leaf hexadecimal-string {
                    nacm:default-deny-all;
                    type yang:hex-string;
                    description
                      "Key in hexadecimal string format.  When
                       compared to ASCII, specification in
                       hexadecimal affords greater key entropy
                       with the same number of internal
                       key-string octets.  Additionally, it
                       discourages usage of well-known words or
                       numbers.";
                  }
                }
              }
            }
            case auth-tls {
              if-feature "tls";
              choice role {
                description
                  "The role of the local entity.";
                case server {
                  container tls-server {
                    uses tlss:tls-server-grouping {
                      description
                        "Server TLS information.";
                    }
                    description
                      "TLS-related information.";
                  }
                }
                case client {
                  container tls-client {
                    uses tlsc:tls-client-grouping {
                      description
                        "Client TLS information.";
                    }
                    description
                      "TLS-related information.";
                  }
                }
              }
            }
          }
        }
      }

      /*
       * Configuration data nodes
       */

      container pcep {
        presence "The PCEP is enabled";
        description
          "Parameters for list of configured PCEP entities
           on the device.";
        container entity {
          description
            "The configured PCEP entity on the device.";
          leaf-list addr {
            type inet:ip-address-no-zone;
            min-elements 1;
            ordered-by user;
            description
              "The local Internet address of this PCEP entity.
               If operating as a PCE server, the PCEP entity
               listens on this address.  If operating as a PCC,
               the PCEP entity binds outgoing TCP connections
               to this address based on the address family.  It is
               possible for the PCEP entity to operate as both a
               PCC and a PCE server, in which case it uses this
               address both to listen for incoming TCP connections
               and to bind outgoing TCP connections.";
          }
          leaf enabled {
            type boolean;
            default "true";
            description
              "The administrative status of this PCEP
               entity; set to true when UP.";
          }
          leaf role {
            type role;
            must '(. != "unknown")' {
              error-message "The PCEP entity role cannot be unknown";
            }
            mandatory true;
            description
              "The role that this entity can play.
               Takes one of the following values:
               - pcc(1): this PCEP entity is a PCC,
               - pce(2): this PCEP entity is a PCE,
               - pcc-and-pce(3): this PCEP entity is both
               a PCC and a PCE.";
          }
          leaf description {
            type string;
            description
              "Description of the PCEP entity configured
               by the user.";
          }
          leaf speaker-entity-id {
            if-feature "sync-opt";
            type string;
            description
              "The Speaker Entity Identifier.";
            reference
              "RFC 8232: Optimizations of Label Switched
               Path State  Synchronization Procedures for
               a Stateful PCE";
          }
          leaf admin-status {
            type boolean;
            default "true";
            description
              "The administrative status of this PCEP entity.
               The value true represents admin status as up.
               This is the desired operational status as
               currently set by an operator or by default in
               the implementation.  The value of oper-status
               represents the current status of an attempt to
               reach this desired status.";
          }
          leaf index {
            type uint32;
            config false;
            description
              "The index of the operational PECP entity.";
          }
          leaf oper-status {
            type oper-status;
            config false;
            description
              "The operational status of the PCEP entity.
               Takes one of the following values:
               - oper-status-up(1): the PCEP entity is active,
               - oper-status-down(2): the PCEP entity is inactive,
               - oper-status-going-up(3): the PCEP entity is
               activating,
               - oper-status-going-down(4): the PCEP entity is
               deactivating,
               - oper-status-failed(5): the PCEP entity has
               failed and will recover when possible,
               - oper-status-failed-perm(6): the PCEP entity
               has failed and will not recover without
               operator intervention.";
          }
          uses domain-info {
            description
              "Local PCEP entity information.";
          }
          uses auth {
            description
              "Local authorization and security parameters.";
          }
          container pce-info {
            when "../role = 'pce'"
               + "or "
               + "../role = 'pcc-and-pce'" {
              description
                "These fields are applicable when the role is PCE.";
            }
            description
              "The local PCE entity PCE information.";
            uses pce-info {
              description
                "Local PCE information.";
            }
            container path-key {
              if-feature "path-key";
              description
                "Path-key configuration.";
              reference
                "RFC 5520: Preserving Topology Confidentiality in
                 Inter-Domain Path Computation Using a Path-Key-
                 Based Mechanism";
              leaf enabled {
                type boolean;
                default "false";
                description
                  "Enabled or disabled; set to true when enabled.";
              }
              leaf discard-timer {
                type uint32;
                units "minutes";
                default "10";
                description
                  "A timer to discard unwanted path-keys.";
              }
              leaf reuse-time {
                type uint32 {
                  range "30..max";
                }
                units "minutes";
                default "30";
                description
                  "A time after which the path-keys could be reused.";
              }
              leaf pce-id {
                type inet:ip-address-no-zone;
                description
                  "PCE address to be used in each Path-Key Subobject
                   (PKS), same as local PCE entity IP address.";
              }
            }
          }
          leaf connect-timer {
            type uint16 {
              range "1..max";
            }
            units "seconds";
            default "60";
            description
              "The time in seconds that the PCEP entity will wait
               to establish a TCP connection with a peer.  If a
               TCP connection is not established within this time,
               then PCEP aborts the session setup attempt.";
            reference
              "RFC 5440: Path Computation Element (PCE) Communication
               Protocol (PCEP)";
          }
          leaf connect-max-retry {
            type uint32;
            default "5";
            description
              "The maximum number of times the system tries to
               establish a TCP connection to a peer before the
               session with the peer transitions to the idle
               state.";
            reference
              "RFC 5440: Path Computation Element (PCE) Communication
               Protocol (PCEP)";
          }
          leaf init-back-off-timer {
            type uint16 {
              range "1..max";
            }
            units "seconds";
            mandatory true;
            description
              "The initial back-off time in seconds for retrying
               a failed session setup attempt to a peer.
               The back-off time increases for each failed
               session setup attempt, until a maximum back-off
               time is reached.  The maximum back-off time is the
               max-back-off-timer leaf.";
            reference
              "RFC 5440: Path Computation Element (PCE) Communication
               Protocol (PCEP)";
          }
          leaf max-back-off-timer {
            type uint32;
            units "seconds";
            mandatory true;
            description
              "The maximum back-off time in seconds for retrying
               a failed session setup attempt to a peer.
               The back-off time increases for each failed session
               setup attempt, until this maximum value is reached.
               Session setup attempts then repeat periodically
               without any further increase in back-off time.";
            reference
              "RFC 5440: Path Computation Element (PCE) Communication
               Protocol (PCEP)";
          }
          leaf open-wait-timer {
            type uint16;
            units "seconds";
            config false;
            description
              "The time in seconds that the PCEP entity will wait
               to receive an Open message from a peer after the
               TCP connection has come up.
               If no Open message is received within this time, then
               PCEP terminates the TCP connection and deletes the
               associated sessions.";
            reference
              "RFC 5440: Path Computation Element (PCE) Communication
               Protocol (PCEP)";
          }
          leaf keep-wait-timer {
            type uint16;
            units "seconds";
            config false;
            description
              "The time in seconds that the PCEP entity will wait
               to receive a Keepalive or PCErr message from a peer
               during session initialization after receiving an
               Open message.  If no Keepalive or PCErr message is
               received within this time, then PCEP terminates the
               TCP connection and deletes the associated
               sessions.";
            reference
              "RFC 5440: Path Computation Element (PCE) Communication
               Protocol (PCEP)";
          }
          leaf keepalive-timer {
            type uint8;
            units "seconds";
            default "30";
            description
              "The Keepalive timer that this PCEP
               entity will propose in the initial Open message of
               each session it is involved in.  This is the
               maximum time between two consecutive messages sent
               to a peer.  Zero means that the PCEP entity prefers
               not to send Keepalives at all.
               Note that the actual Keepalive transmission
               intervals, in either direction of an active PCEP
               session, are determined by negotiation between the
               peers as specified by RFC 5440 and thus may differ
               from this configured value.";
            reference
              "RFC 5440: Path Computation Element (PCE) Communication
               Protocol (PCEP)";
          }
          leaf dead-timer {
            type uint8;
            units "seconds";
            must '(. > ../keepalive-timer)' {
              error-message "The DeadTimer must be "
                          + "larger than the Keepalive timer";
            }
            default "120";
            description
              "The DeadTimer that this PCEP entity will propose
               in the initial Open message of each session it is
               involved in.  This is the time after which a peer
               should declare a session down if it does not
               receive any PCEP messages.  Zero suggests that the
               peer does not run a DeadTimer at all.";
            reference
              "RFC 5440: Path Computation Element (PCE) Communication
               Protocol (PCEP)";
          }
          leaf allow-negotiation {
            type boolean;
            default "true";
            description
              "Whether the PCEP entity will permit the negotiation
               of session parameters.";
          }
          leaf max-keepalive-timer {
            type uint8;
            units "seconds";
            mandatory true;
            description
              "The maximum value that this PCEP entity will
               accept from a peer for the interval between
               Keepalive transmissions.  Zero means that the PCEP
               entity will allow no Keepalive transmission at
               all.";
          }
          leaf max-dead-timer {
            type uint8;
            units "seconds";
            mandatory true;
            description
              "The maximum value in seconds that this PCEP
               entity will accept from a peer for the DeadTimer.
               Zero means that the PCEP entity will allow not
               running a DeadTimer.";
          }
          leaf min-keepalive-timer {
            type uint8;
            units "seconds";
            mandatory true;
            description
              "The minimum value in seconds that this PCEP
               entity will accept for the interval between
               Keepalive transmissions.  Zero means that the
               PCEP entity insists on no Keepalive
               transmission at all.";
          }
          leaf min-dead-timer {
            type uint8;
            units "seconds";
            mandatory true;
            description
              "The minimum value in seconds that this PCEP
               entity will accept for the DeadTimer.  Zero
               means that the PCEP entity insists on not
               running a DeadTimer.";
          }
          leaf sync-timer {
            if-feature "svec";
            type uint16;
            units "seconds";
            default "60";
            description
              "The value of SyncTimer in seconds is used in the
               case of synchronized path computation request
               using the SVEC object.  If after the expiration of
               the SyncTimer all the path computation requests
               have not been received, a protocol error is
               triggered, and the PCE must cancel the whole set
               of path computation requests.
               Zero means that the PCEP entity does not use the
               SyncTimer.";
            reference
              "RFC 5440: Path Computation Element (PCE)
               Communication Protocol (PCEP)";
          }
          leaf request-timer {
            type uint16 {
              range "1..max";
            }
            units "seconds";
            mandatory true;
            description
              "The maximum time that the PCEP entity will wait
               for a response to a PCReq message.";
          }
          leaf max-sessions {
            type uint32;
            mandatory true;
            description
              "Maximum number of sessions involving this PCEP
               entity that can exist at any time.";
          }
          leaf max-unknown-reqs {
            type uint32;
            default "5";
            description
              "The maximum number of unrecognized requests and
               replies that any session on this PCEP entity is
               willing to accept per minute before terminating
               the session.
               A PCRep message contains an unrecognized reply
               if it contains an RP object whose request ID
               does not correspond to any in-progress request
               sent by this PCEP entity.
               A PCReq message contains an unrecognized request
               if it contains an RP object whose request ID is
               zero.";
            reference
              "RFC 5440: Path Computation Element (PCE)
               Communication Protocol (PCEP)";
          }
          leaf max-unknown-msgs {
            type uint32;
            default "5";
            description
              "The maximum number of unknown messages that any
               session on this PCEP entity is willing to accept
               per minute before terminating the session.";
            reference
              "RFC 5440: Path Computation Element (PCE)
               Communication Protocol (PCEP)";
          }
          leaf pcep-notification-max-rate {
            type uint32;
            mandatory true;
            description
              "This variable indicates the maximum number of
               notifications issued per second.  If events
               occur more rapidly, the implementation may
               simply fail to emit these notifications during
               that period or may queue them until an
               appropriate time.  A value of 0 means no
               notifications are emitted and all should be
               discarded (that is, not queued).";
          }
          container stateful-parameter {
            if-feature "stateful";
            description
              "The configured stateful PCE parameters.";
            leaf state-timeout {
              type uint32;
              units "seconds";
              mandatory true;
              description
                "When a PCEP session is terminated, a PCC
                 waits for this time period before flushing
                 LSP state associated with that PCEP session
                 and reverting to operator-defined default
                 parameters or behaviors.  The max value
                 represents infinity.";
              reference
                "RFC 8231: Path Computation Element Communication
                 Protocol (PCEP) Extensions for Stateful PCE";
            }
            leaf redelegation-timeout {
              when "../../role = 'pcc'"
                 + "or "
                 + "../../role = 'pcc-and-pce'" {
                description
                  "This field is applicable when the role is
                   PCC.";
              }
              type uint32;
              units "seconds";
              must '(. < ../state-timeout)' {
                error-message "The Redelegation Timeout must be "
                            + "less than the State Timeout";
              }
              mandatory true;
              description
                "When a PCEP session is terminated, a PCC
                 waits for this time period before revoking
                 LSP delegation to a PCE and attempting to
                 redelegate LSPs associated with the
                 terminated PCEP session to an alternate
                 PCE.";
              reference
                "RFC 8231: Path Computation Element Communication
                 Protocol (PCEP) Extensions for Stateful PCE";
            }
            leaf rpt-non-pcep-lsp {
              when "../../role = 'pcc'"
                 + "or "
                 + "../../role = 'pcc-and-pce'" {
                description
                  "This field is applicable when the role is
                   PCC.";
              }
              type boolean;
              default "true";
              description
                "If set, a PCC reports LSPs that are not
                 controlled by any PCE (for example, LSPs
                 that are statically configured at the
                 PCC).";
            }
            reference
              "RFC 8231: Path Computation Element Communication Protocol
               (PCEP) Extensions for Stateful PCE";
          }
          container of-list {
            when "../role = 'pce'"
               + "or "
               + "../role = 'pcc-and-pce'" {
              description
                "These fields are applicable when the role is
                 PCE.";
            }
            if-feature "objective-function";
            uses of-list;
            description
              "The authorized OF-List at PCE for all peers.";
          }
          container lsp-db {
            if-feature "stateful";
            config false;
            description
              "The LSP-DB.";
            leaf db-ver {
              when "../../role = 'pcc'"
                 + "or "
                 + "../../role = 'pcc-and-pce'" {
                description
                  "This field is applicable when the role is
                   PCC.";
              }
              if-feature "sync-opt";
              type uint64;
              description
                "The LSP State Database Version Number.";
            }
            list association-list {
              if-feature "association";
              key "type id source global-source extended-id";
              description
                "List of all PCEP associations.";
              reference
                "RFC 8697: Path Computation Element Communication
                 Protocol (PCEP) Extensions for Establishing
                 Relationships between Sets of Label Switched
                 Paths (LSPs)";
              leaf type {
                type identityref {
                  base te-types:association-type;
                }
                description
                  "The PCEP Association Type.";
                reference
                  "IANA PCEP: ASSOCIATION Type Field in Path
                   Computation Element Protocol (PCEP) Numbers
                   RFC 8697: Path Computation Element Communication
                   Protocol (PCEP) Extensions for Establishing
                   Relationships between Sets of Label Switched
                   Paths (LSPs)";
              }
              leaf id {
                type uint16;
                description
                  "PCEP Association ID.";
              }
              leaf source {
                type inet:ip-address-no-zone;
                description
                  "PCEP Association Source.";
              }
              leaf global-source {
                type uint32;
                description
                  "PCEP Global Association Source.";
              }
              leaf extended-id {
                type string;
                description
                  "Additional information to support unique
                   identification (Extended Association ID).";
              }
              list lsp {
                key "plsp-id pcc-id lsp-id";
                description
                  "List of all LSP in this association.";
                leaf plsp-id {
                  type leafref {
                    path "/pcep/entity/lsp-db/"
                       + "lsp/plsp-id";
                  }
                  description
                    "Reference to PLSP-ID in LSP-DB.";
                }
                leaf pcc-id {
                  type leafref {
                    path "/pcep/entity/lsp-db/"
                       + "lsp[plsp-id=current()/"
                       + "../plsp-id]/pcc-id";
                  }
                  description
                    "Reference to PCC-ID in LSP-DB.";
                }
                leaf lsp-id {
                  type leafref {
                    path "/pcep/entity/lsp-db/"
                       + "lsp[plsp-id=current()/../plsp-id]"
                       + "[pcc-id=current()/../pcc-id]/lsp-id";
                  }
                  description
                    "Reference to LSP-ID in LSP-DB.";
                }
              }
            }
            list lsp {
              key "plsp-id pcc-id lsp-id";
              description
                "List of all LSPs in LSP-DB.";
              leaf plsp-id {
                type uint32 {
                  range "1..1048575";
                }
                description
                  "A PCEP-specific identifier for the LSP.  A PCC
                   creates a unique PLSP-ID for each LSP that is
                   constant for the lifetime of a PCEP session.
                   PLSP-ID is 20 bits with 0 and 0xFFFFF
                   reserved.";
              }
              leaf pcc-id {
                type inet:ip-address-no-zone;
                description
                  "The local IP address of the PCC that
                   generated the PLSP-ID.";
              }
              leaf source {
                type inet:ip-address-no-zone;
                description
                  "Tunnel sender address extracted from
                   LSP-IDENTIFIERS TLV.";
                reference
                  "RFC 8231: Path Computation Element
                   Communication Protocol (PCEP) Extensions
                   for Stateful PCE";
              }
              leaf destination {
                type inet:ip-address-no-zone;
                description
                  "Tunnel endpoint address extracted from
                   LSP-IDENTIFIERS TLV.";
                reference
                  "RFC 8231: Path Computation Element
                   Communication Protocol (PCEP) Extensions
                   for Stateful PCE";
              }
              leaf tunnel-id {
                type uint16;
                description
                  "Tunnel identifier used in the LSP-IDENTIFIERS
                   TLV that remains constant over the life
                   of the tunnel.";
                reference
                  "RFC 8231: Path Computation Element
                   Communication Protocol (PCEP) Extensions
                   for Stateful PCE";
              }
              leaf lsp-id {
                type uint16;
                description
                  "Identifier used in the LSP-IDENTIFIERS TLV
                   that can be changed to allow a sender to share
                   resources with itself.";
                reference
                  "RFC 8231: Path Computation Element
                   Communication Protocol (PCEP) Extensions
                   for Stateful PCE";
              }
              leaf extended-tunnel-id {
                type inet:ip-address-no-zone;
                description
                  "Extended tunnel ID of the LSP in LSP-IDENTIFIERS
                   TLV. The all-zeros format is represented as
                   0.0.0.0 and ::.";
                reference
                  "RFC 8231: Path Computation Element
                   Communication Protocol (PCEP) Extensions
                   for Stateful PCE";
              }
              leaf admin-state {
                type boolean;
                default "true";
                description
                  "The desired operational state.";
              }
              leaf operational-state {
                type operational-state;
                description
                  "The operational status of the LSP.";
              }
              container delegated {
                description
                  "The delegation-related parameters.";
                leaf enabled {
                  type boolean;
                  default "false";
                  description
                    "LSP is delegated or not; set to true when
                     delegated.";
                }
                leaf peer {
                  when '../enabled' {
                    description
                      "The LSP must be delegated.";
                  }
                  type leafref {
                    path "/pcep/entity/peers/peer/addr";
                  }
                  description
                    "At the PCC, the reference to the PCEP peer to
                     which LSP is delegated; at the PCE, the
                     reference to the PCEP peer that delegated this
                     LSP.";
                }
                leaf srp-id {
                  type uint32 {
                    range "1..4294967294";
                  }
                  description
                    "The last SRP-ID-number associated with this
                     LSP.  The values 0x00000000 and 0xFFFFFFFF
                     are reserved.";
                }
              }
              container initiation {
                if-feature "pce-initiated";
                description
                  "The parameters related to PCE initiation.";
                reference
                  "RFC 8281: Path Computation Element Communication
                   Protocol (PCEP) Extensions for PCE-Initiated LSP
                   Setup in a Stateful PCE Model";
                leaf enabled {
                  type boolean;
                  default "false";
                  description
                    "Set to true if this LSP is initiated by a PCE.";
                }
                leaf peer {
                  when '../enabled' {
                    description
                      "The LSP must be PCE-initiated.";
                  }
                  type leafref {
                    path "/pcep/entity/peers/peer/addr";
                  }
                  description
                    "If the role is PCC, this leaf refers to the PCEP
                     peer (PCE) that initiated this LSP.  If the role
                     is PCE, this leaf refers to the PCEP peer (PCC)
                     where the LSP is initiated.";
                }
              }
              leaf symbolic-path-name {
                type string;
                description
                  "The symbolic path name associated with the LSP.";
                reference
                  "RFC 8231: Path Computation Element Communication
                   Protocol (PCEP) Extensions for Stateful PCE";
              }
              leaf last-error {
                type identityref {
                  base lsp-error;
                }
                description
                  "The last error for the LSP.";
              }
              leaf pst {
                type identityref {
                  base te-types:path-signaling-type;
                }
                default "te-types:path-setup-rsvp";
                description
                  "The Path Setup Type (PST).  Note that the
                   te-types model uses the term Path Signaling
                   Type.";
                reference
                  "RFC 8408: Conveying Path Setup Type in PCE
                   Communication Protocol (PCEP) Messages";
              }
              list association-list {
                if-feature "association";
                key "type id source global-source extended-id";
                description
                  "List of all PCEP associations.";
                leaf type {
                  type leafref {
                    path "/pcep/entity/lsp-db/"
                       + "association-list/type";
                  }
                  description
                    "PCEP Association Type.";
                }
                leaf id {
                  type leafref {
                    path "/pcep/entity/lsp-db/"
                       + "association-list[type=current()/"
                       + "../type]/id";
                  }
                  description
                    "PCEP Association ID.";
                }
                leaf source {
                  type leafref {
                    path "/pcep/entity/lsp-db/"
                       + "association-list[type=current()/../type]"
                       + "[id=current()/../id]/source";
                  }
                  description
                    "PCEP Association Source.";
                }
                leaf global-source {
                  type leafref {
                    path "/pcep/entity/lsp-db/"
                       + "association-list[type=current()/../type]"
                       + "[id=current()/../id]"
                       + "[source=current()/../source]"
                       + "/global-source";
                  }
                  description
                    "PCEP Global Association Source.";
                }
                leaf extended-id {
                  type leafref {
                    path "/pcep/entity/lsp-db/"
                       + "association-list[type=current()/../type]"
                       + "[id=current()/../id]"
                       + "[source=current()/../source]"
                       + "[global-source=current()/../global-source]"
                       + "/extended-id";
                  }
                  description
                    "Additional information to
                     support unique identification.";
                }
                reference
                  "RFC 8697: Path Computation Element Communication
                   Protocol (PCEP) Extensions for Establishing
                   Relationships between Sets of Label Switched
                   Paths (LSPs)";
              }
            }
          }
          container path-keys {
            when "../role = 'pce' or ../role = 'pcc-and-pce'" {
              description
                "These fields are applicable when the role is
                 PCE.";
            }
            if-feature "path-key";
            config false;
            description
              "The path-keys generated by the PCE.";
            reference
              "RFC 5520: Preserving Topology Confidentiality
               in Inter-Domain Path Computation Using a Path-
               Key-Based Mechanism";
            list path-key {
              key "key";
              description
                "The list of path-keys generated by the PCE.";
              leaf key {
                type uint16;
                description
                  "The identifier or token used to represent
                   the Confidential Path Segment (CPS) within
                   the context of the PCE.";
              }
              container cps {
                description
                  "The Confidential Path Segment (CPS).";
                list explicit-route-objects {
                  key "index";
                  description
                    "List of Explicit Route Objects (EROs).";
                  leaf index {
                    type uint32;
                    description
                      "ERO subobject index.";
                  }
                  uses te-types:explicit-route-hop;
                }
              }
              leaf pcc-requester {
                type leafref {
                  path "/pcep/entity/peers/peer/addr";
                }
                description
                  "Reference to PCC peer address that
                   issued the original request that led
                   to the creation of the path-key.";
              }
              leaf req-id {
                type uint32;
                description
                  "The request ID of the original PCReq.";
              }
              leaf retrieved {
                type boolean;
                description
                  "If path-key has been retrieved yet.";
              }
              leaf pcc-retrieved {
                when '../retrieved' {
                  description
                    "The path-key should be retrieved.";
                }
                type leafref {
                  path "/pcep/entity/peers/peer/addr";
                }
                description
                  "Reference to PCC peer address that
                   retrieved the path-key.";
              }
              leaf creation-time {
                type yang:timestamp;
                description
                  "The timestamp value at the time this path-key
                   was created.";
              }
              leaf discard-time {
                type uint32;
                units "minutes";
                description
                  "A time after which this path-key will be
                   discarded.";
              }
              leaf reuse-time {
                type uint32;
                units "minutes";
                description
                  "A time after which this path-key could be
                   reused.";
              }
            }
          }
          container peers {
            description
              "The list of configured peers for the
               entity (remote PCE).";
            list peer {
              key "addr";
              description
                "The peer configured for the entity.
                 (remote PCE).";
              leaf addr {
                type inet:ip-address-no-zone;
                description
                  "The local Internet address of this
                   PCEP peer.";
              }
              leaf role {
                type role;
                must '(. != "pcc-and-pce")' {
                  error-message
                    "The PCEP peer cannot be both
                     PCE and PCC at the same time";
                }
                mandatory true;
                description
                  "The role of the PCEP peer.
                   Takes one of the following values:
                   - unknown(0): this PCEP peer role is not
                   known,
                   - pcc(1): this PCEP peer is a PCC,
                   - pce(2): this PCEP peer is a PCE,
                   - pcc-and-pce(3): is not allowed as PCEP
                   peer cannot be acting as both a PCC and a
                   PCE at the same time.";
              }
              leaf description {
                type string;
                description
                  "Description of the PCEP peer
                   configured by the user.";
              }
              uses domain-info {
                description
                  "PCE peer information.";
              }
              container pce-info {
                uses pce-info {
                  description
                    "Using the PCE peer information grouping.";
                }
                description
                  "The PCE peer information.";
              }
              leaf delegation-pref {
                if-feature "stateful";
                type uint8 {
                  range "0..7";
                }
                mandatory true;
                description
                  "The PCE peer delegation preference, where
                   7 reflects the highest preference.";
              }
              uses auth {
                description
                  "The PCE peer authorization and security
                   parameters.";
              }
              leaf discontinuity-time {
                type yang:timestamp;
                config false;
                description
                  "The timestamp of the time when the information and
                   statistics were last reset.";
              }
              leaf initiate-session {
                type boolean;
                config false;
                description
                  "Indicates whether the local PCEP entity initiates
                   sessions to this peer or waits for the peer to
                   initiate a session.";
              }
              leaf session-exists {
                type boolean;
                config false;
                description
                  "Indicates whether a session with
                   this peer currently exists.";
              }
              leaf session-up-time {
                type yang:timestamp;
                config false;
                description
                  "The timestamp value of the last time a
                   session with this peer was successfully
                   established.";
              }
              leaf session-fail-time {
                type yang:timestamp;
                config false;
                description
                  "The timestamp value of the last time a
                   session with this peer failed to be
                   established.";
              }
              leaf session-fail-up-time {
                type yang:timestamp;
                config false;
                description
                  "The timestamp value of the last time a
                   session with this peer failed from
                   active.";
              }
              container sessions {
                config false;
                description
                  "This entry represents a single PCEP
                   session in which the local PCEP entity participates.
                   This entry exists only if the corresponding PCEP
                   session has been initialized by some event, such as
                   manual user configuration, auto-discovery of a peer,
                   or an incoming TCP connection.";
                list session {
                  key "initiator";
                  description
                    "The list of sessions; note that for a time being
                     two sessions may exist for a peer.";
                  leaf initiator {
                    type initiator;
                    description
                      "The initiator of the session, that is, whether
                       the TCP connection was initiated by the local
                       PCEP entity or the peer.
                       There is a window during session
                       initialization where two sessions can exist
                       between a pair of PCEP speakers, each
                       initiated by one of the speakers.  One of
                       these sessions is always discarded before it
                       leaves OpenWait state.  However, before it is
                       discarded, two sessions to the given peer
                       appear transiently in this YANG module.  The
                       sessions are distinguished by who initiated
                       them, and so this field is the key.";
                  }
                  leaf role {
                    type leafref {
                      path "../../../role";
                    }
                    description
                      "The peer role.";
                  }
                  leaf state-last-change {
                    type yang:timestamp;
                    description
                      "The timestamp value at the time this
                       session entered its current state as
                       denoted by the state leaf.";
                  }
                  leaf state {
                    type sess-state;
                    description
                      "The current state of the session.
                       The set of possible states excludes the
                       idle state since entries do not exist
                       in the idle state.";
                  }
                  leaf session-creation {
                    type yang:timestamp;
                    description
                      "The timestamp value at the time this
                       session was created.";
                  }
                  leaf connect-retry {
                    type yang:counter32;
                    description
                      "The number of times that the local PCEP
                       entity has attempted to establish a TCP
                       connection for this session without
                       success.  The PCEP entity gives up when
                       this reaches connect-max-retry.";
                  }
                  leaf local-id {
                    type uint8;
                    description
                      "The value of the PCEP session ID used by
                       the local PCEP entity in the Open message
                       for this session. If the state is tcp-pending,
                       then this is the session ID that will be
                       used in the Open message.  Otherwise, this
                       is the session ID that was sent in the
                       Open message.";
                    reference
                      "RFC 5440: Path Computation Element (PCE)
                       Communication Protocol (PCEP)";
                  }
                  leaf remote-id {
                    type uint8;
                    description
                      "The value of the PCEP session ID used by the
                       peer in its Open message for this session.

                       If the state is TCPPending or OpenWait, then
                       this leaf is not used and MUST be set to
                       zero.";
                    reference
                      "RFC 5440: Path Computation Element (PCE)
                       Communication Protocol (PCEP)";
                  }
                  leaf keepalive-timer {
                    type uint8;
                    units "seconds";
                    description
                      "The agreed maximum interval at which the local
                       PCEP entity transmits PCEP messages on this PCEP
                       session.  Zero means that the local PCEP entity
                       never sends Keepalives on this session.

                       This field is used if and only if the state
                       is session-up.  Otherwise, it is not used and
                       MUST be set to zero.";
                    reference
                      "RFC 5440: Path Computation Element (PCE)
                       Communication Protocol (PCEP)";
                  }
                  leaf peer-keepalive-timer {
                    type uint8;
                    units "seconds";
                    description
                      "The agreed maximum interval at which the peer
                       transmits PCEP messages on this PCEP session.
                       Zero means that the peer never sends Keepalives
                       on this session.

                       This field is used if and only if state is
                       session-up.  Otherwise, it is not used and MUST
                       be set to zero.";
                    reference
                      "RFC 5440: Path Computation Element (PCE)
                       Communication Protocol (PCEP)";
                  }
                  leaf dead-timer {
                    type uint8;
                    units "seconds";
                    description
                      "The DeadTimer interval for this PCEP session.";
                    reference
                      "RFC 5440: Path Computation Element (PCE)
                       Communication Protocol (PCEP)";
                  }
                  leaf peer-dead-timer {
                    type uint8;
                    units "seconds";
                    description
                      "The peer's DeadTimer interval for this PCEP
                       session.

                       If the state is TCPPending or OpenWait, then
                       this leaf is not used and MUST be set to zero.";
                    reference
                      "RFC 5440: Path Computation Element (PCE)
                       Communication Protocol (PCEP)";
                  }
                  leaf ka-hold-time-rem {
                    type uint8;
                    units "seconds";
                    description
                      "The Keepalive hold time remaining for this
                       session.

                       If the state is TCPPending or OpenWait, then
                       this field is not used and MUST be set to
                       zero.";
                  }
                  leaf overloaded {
                    type boolean;
                    description
                      "If the local PCEP entity has informed the peer
                       that it is currently overloaded, then this is
                       set to true.  Otherwise, it is set to false.";
                    reference
                      "RFC 5440: Path Computation Element (PCE)
                       Communication Protocol (PCEP)";
                  }
                  leaf overloaded-timestamp {
                    when '../overloaded' {
                      description
                        "Valid when overloaded.";
                    }
                    type yang:timestamp;
                    description
                      "The timestamp value of the time when the
                       overloaded field was set to true.";
                  }
                  leaf overload-time {
                    type uint32;
                    units "seconds";
                    description
                      "The interval of time that is remaining until the
                       local PCEP entity will cease to be overloaded on
                       this session.

                       This field is only used if overloaded is set to
                       true.  Otherwise, it is not used and MUST be set
                       to zero.";
                    reference
                      "RFC 5440: Path Computation Element (PCE)
                       Communication Protocol (PCEP)";
                  }
                  leaf peer-overloaded {
                    type boolean;
                    description
                      "If the peer has informed the local PCEP entity
                       that it is currently overloaded, then this is
                       set to true.  Otherwise, it is set to false.";
                    reference
                      "RFC 5440: Path Computation Element (PCE)
                       Communication Protocol (PCEP)";
                  }
                  leaf peer-overloaded-timestamp {
                    when '../peer-overloaded' {
                      description
                        "Valid when peer is overloaded.";
                    }
                    type yang:timestamp;
                    description
                      "The timestamp value of the time when the
                       peer-overloaded field was set to true.";
                  }
                  leaf peer-overload-time {
                    type uint32;
                    units "seconds";
                    description
                      "The interval of time that is remaining until
                       the peer will cease to be overloaded.  If it
                       is not known how long the peer will stay in
                       overloaded state, this leaf is set to zero.

                       This field is only used if peer-overloaded
                       is set to true.  Otherwise, it is not used
                       and MUST be set to zero.";
                    reference
                      "RFC 5440: Path Computation Element (PCE)
                       Communication Protocol (PCEP)";
                  }
                  leaf lspdb-sync {
                    if-feature "stateful";
                    type sync-state;
                    description
                      "The LSP-DB state synchronization status.";
                    reference
                      "RFC 8231: Path Computation Element Communication
                       Protocol (PCEP) Extensions for Stateful PCE";
                  }
                  leaf recv-db-ver {
                    when "../role = 'pcc'"
                       + "or "
                       + "../role = 'pcc-and-pce'" {
                      description
                        "This field is applicable when the role is
                         PCC.";
                    }
                    if-feature "stateful";
                    if-feature "sync-opt";
                    type uint64;
                    description
                      "The last received LSP State Database Version
                       Number.";
                    reference
                      "RFC 8231: Path Computation Element Communication
                       Protocol (PCEP) Extensions for Stateful PCE";
                  }
                  container of-list {
                    when "../role = 'pce'"
                       + "or "
                       + "../role = 'pcc-and-pce'" {
                      description
                        "These fields are applicable when the role is
                         PCE.";
                    }
                    if-feature "objective-function";
                    uses of-list;
                    description
                      "Indicate the list of supported OF on this
                       session.";
                    reference
                      "RFC 5541: Encoding of Objective Functions in
                       the Path  Computation Element Communication
                       Protocol (PCEP)";
                  }
                  container pst-list {
                    when "../role = 'pce'"
                       + "or "
                       + "../role = 'pcc-and-pce'" {
                      description
                        "These fields are applicable when the role is
                         PCE.";
                    }
                    description
                      "Indicate the list of supported
                       PST on this session.";
                    reference
                      "RFC 8408: Conveying Path Setup Type in PCE
                       Communication Protocol (PCEP) Messages";
                    list path-setup-type {
                      key "pst";
                      description
                        "The list of PST.";
                      leaf pst {
                        type identityref {
                          base te-types:path-signaling-type;
                        }
                        description
                          "The PST supported.";
                      }
                    }
                  }
                  container assoc-type-list {
                    if-feature "association";
                    description
                      "Indicate the list of supported association types
                       on this session.";
                    reference
                      "RFC 8697: Path Computation Element Communication
                       Protocol (PCEP) Extensions for Establishing
                       Relationships between Sets of Label Switched
                       Paths (LSPs)";
                    list assoc-type {
                      key "at";
                      description
                        "The list of authorized association types.";
                      leaf at {
                        type identityref {
                          base te-types:association-type;
                        }
                        description
                          "The association type authorized.";
                      }
                    }
                  }
                  leaf speaker-entity-id {
                    if-feature "sync-opt";
                    type string;
                    description
                      "The Speaker Entity Identifier.";
                    reference
                      "RFC 8232: Optimizations of Label Switched
                       Path State  Synchronization Procedures for
                       a Stateful PCE";
                  }
                }
              }
            }
          }
        }
      }

      /*
       * Notifications
       */

      notification pcep-session-up {
        description
          "This notification is sent when the value of
           '/pcep/peers/peer/sessions/session/state'
           enters the 'session-up' state.";
        uses notification-session-hdr;
        leaf state-last-change {
          type yang:timestamp;
          description
            "The timestamp value at the time this session
             entered its current state as denoted by the state
             leaf.";
        }
        leaf state {
          type sess-state;
          description
            "The current state of the session.
             The set of possible states excludes the idle state
             since entries do not exist in the idle state.";
        }
        reference
          "RFC 5440: Path Computation Element (PCE) Communication
           Protocol (PCEP)";
      }

      notification pcep-session-down {
        description
          "This notification is sent when the value of
           '/pcep/peers/peer/sessions/session/state'
           leaves the 'session-up' state.";
        uses notification-instance-hdr;
        leaf session-initiator {
          type initiator;
          description
            "The initiator of the session.";
        }
        leaf state-last-change {
          type yang:timestamp;
          description
            "The timestamp value at the time this session
             entered its current state as denoted by the state
             leaf.";
        }
        leaf state {
          type sess-state;
          description
            "The current state of the session.
             The set of possible states excludes the idle state
             since entries do not exist in the idle state.";
        }
        reference
          "RFC 5440: Path Computation Element (PCE) Communication
           Protocol (PCEP)";
      }

      notification pcep-session-local-overload {
        description
          "This notification is sent when the local PCEP entity
           enters overload state for a peer.";
        uses notification-session-hdr;
        leaf overloaded {
          type boolean;
          description
            "If the local PCEP entity has informed the peer
             that it is currently overloaded, then this is set
             to true.  Otherwise, it is set to false.";
        }
        leaf overloaded-timestamp {
          type yang:timestamp;
          description
            "The timestamp value of the time when the
             overloaded field was set to true.";
        }
        leaf overload-time {
          type uint32;
          units "seconds";
          description
            "The interval of time that is remaining until the
             local PCEP entity will cease to be overloaded on
             this session.";
        }
        reference
          "RFC 5440: Path Computation Element (PCE) Communication
           Protocol (PCEP)";
      }

      notification pcep-session-local-overload-clear {
        description
          "This notification is sent when the local PCEP entity
           leaves overload state for a peer.";
        uses notification-instance-hdr;
        leaf overloaded {
          type boolean;
          description
            "If the local PCEP entity has informed the peer
             that it is currently overloaded, then this is set
             to true.  Otherwise, it is set to false.";
        }
        leaf overloaded-clear-timestamp {
          type yang:timestamp;
          description
            "The timestamp value of the time when the
             overloaded field was set to false.";
        }
        reference
          "RFC 5440: Path Computation Element (PCE) Communication
           Protocol (PCEP)";
      }

      notification pcep-session-peer-overload {
        description
          "This notification is sent when a peer enters overload
           state.";
        uses notification-session-hdr;
        leaf peer-overloaded {
          type boolean;
          description
            "If the peer has informed the local PCEP entity that
             it is currently overloaded, then this is set to
             true.  Otherwise, it is set to false.";
        }
        leaf peer-overloaded-timestamp {
          type yang:timestamp;
          description
            "The timestamp value of the time when the
             peer-overloaded field was set to true.";
        }
        leaf peer-overload-time {
          type uint32;
          units "seconds";
          description
            "The interval of time that is remaining until the
             peer will cease to be overloaded.  If it is not
             known how long the peer will stay in overloaded
             state, this leaf is set to zero.";
        }
        reference
          "RFC 5440: Path Computation Element (PCE) Communication
           Protocol (PCEP)";
      }

      notification pcep-session-peer-overload-clear {
        description
          "This notification is sent when a peer leaves overload
           state.";
        uses notification-instance-hdr;
        leaf peer-overloaded {
          type boolean;
          description
            "If the peer has informed the local PCEP entity that
             it is currently overloaded, then this is set to
             true.  Otherwise, it is set to false.";
        }
        leaf peer-overloaded-clear-timestamp {
          type yang:timestamp;
          description
            "The timestamp value of the time when the
             peer-overloaded field was set to false.";
        }
        reference
          "RFC 5440: Path Computation Element (PCE) Communication
           Protocol (PCEP)";
      }

      /*
       * RPC
       */

      rpc trigger-resync {
        if-feature "stateful";
        if-feature "sync-opt";
        nacm:default-deny-all;
        description
          "Trigger the resynchronization at the PCE.";
        reference
          "RFC 8232: Optimizations of Label Switched Path State
           Synchronization Procedures for a Stateful PCE";
        input {
          leaf pcc {
            type leafref {
              path "/pcep/entity/peers/peer/addr";
            }
            mandatory true;
            description
              "The IP address to identify the PCC.  The state
               synchronization is re-triggered for all LSPs from
               the PCC.  The rpc on the PCC will be ignored.";
          }
        }
      }
    }

    <CODE ENDS>

¶

### 8.2. ietf-pcep-stats Module

    <CODE BEGINS> file "ietf-pcep-stats@2025-09-12.yang"

    module ietf-pcep-stats {
      yang-version 1.1;
      namespace "urn:ietf:params:xml:ns:yang:ietf-pcep-stats";
      prefix pcep-stats;

      import ietf-pcep {
        prefix pcep;
        reference
          "RFC 9826: A YANG Data Model for the Path Computation
           Element Communication Protocol (PCEP)";
      }
      import ietf-yang-types {
        prefix yang;
        reference
          "RFC 6991: Common YANG Data Types";
      }

      organization
        "IETF PCE (Path Computation Element) Working Group";
      contact
        "WG Web:  <https://datatracker.ietf.org/wg/pce/>
         WG List:  <mailto:pce@ietf.org>
         Editor:   Dhruv Dhody
                  <mailto:dhruv.ietf@gmail.com>";
      description
        "The YANG module augments the Path Computation Element
         Communication Protocol (PCEP) YANG operational
         model with statistics, counters and telemetry data.

         Copyright (c) 2025 IETF Trust and the persons identified as
         authors of the code.  All rights reserved.

         Redistribution and use in source and binary forms, with or
         without modification, is permitted pursuant to, and subject to
         the license terms contained in, the Revised BSD License set
         forth in Section 4.c of the IETF Trust's Legal Provisions
         Relating to IETF Documents
         (https://trustee.ietf.org/license-info).

         This version of this YANG module is part of RFC 9826; see the
         RFC itself for full legal notices.";

      revision 2025-09-12 {
        description
          "Initial revision.";
        reference
          "RFC 9826: A YANG Data Model for the Path Computation
           Element Communication Protocol (PCEP)";
      }

      /*
       * Features
       */

      feature reset-all {
        description
          "Support resetting of all PCEP statistics.";
      }

      /*
       * Groupings
       */

      grouping stats {
        description
          "This grouping defines statistics for PCEP.  It is used
           for both peer and current sessions.  Since this grouping
           includes a relative path, care needs to be taken while
           using it.";
        leaf discontinuity-time {
          type yang:timestamp;
          description
            "The timestamp value of the time when the
             statistics were last reset.";
        }
        container pce {
          when "../../pcep:role = 'pce'"
             + "or "
             + "../../pcep:role = 'pcc-and-pce'" {
            description
              "Valid for PCEP peer as PCE.";
          }
          leaf rsp-time-avg {
            type uint32;
            units "milliseconds";
            description
              "The average response time.  If an average response time
               has not been calculated, then this leaf has the value
               zero.";
          }
          leaf rsp-time-lwm {
            type uint32;
            units "milliseconds";
            description
              "The smallest (low-water mark) response time seen.
               If no responses have been received, then this leaf has
               the value zero.";
          }
          leaf rsp-time-hwm {
            type uint32;
            units "milliseconds";
            description
              "The greatest (high-water mark) response time seen.
               If no responses have been received, then this object
               has the value zero.";
          }
          leaf pcreq-sent {
            type yang:counter32;
            description
              "The number of PCReq messages sent.";
          }
          leaf pcreq-rcvd {
            type yang:counter32;
            description
              "The number of PCReq messages received.";
          }
          leaf pcrep-sent {
            type yang:counter32;
            description
              "The number of PCRep messages sent.";
          }
          leaf pcrep-rcvd {
            type yang:counter32;
            description
              "The number of PCRep messages received.";
          }
          leaf req-sent {
            type yang:counter32;
            description
              "The number of requests sent.  A request corresponds
               1:1 with an RP object in a PCReq message.  This might
               be greater than pcreq-sent because multiple
               requests can be batched into a single PCReq
               message.";
          }
          leaf req-sent-pend-rep {
            type yang:counter32;
            description
              "The number of requests that have been sent for
               which a response is still pending.";
          }
          leaf req-sent-ero-rcvd {
            type yang:counter32;
            description
              "The number of requests that have been sent for
               which a response with an ERO object was received.
               Such responses indicate that a path was
               successfully computed by the peer.";
          }
          leaf req-sent-nopath-rcvd {
            type yang:counter32;
            description
              "The number of requests that have been sent for
               which a response with a NO-PATH object was
               received.  Such responses indicate that the peer
               could not find a path to satisfy the
               request.";
          }
          leaf req-sent-cancel-rcvd {
            type yang:counter32;
            description
              "The number of requests that were cancelled with
               a PCNtf message.  This might be different than
               pcntf-rcvd because not all PCNtf messages are
               used to cancel requests, and a single PCNtf message
               can cancel multiple requests.";
          }
          leaf req-sent-error-rcvd {
            type yang:counter32;
            description
              "The number of requests that were rejected with a
               PCErr message.  This might be different than
               pcerr-rcvd because not all PCErr messages are
               used to reject requests, and a single PCErr message
               can reject multiple requests.";
          }
          leaf req-sent-timeout {
            type yang:counter32;
            description
              "The number of requests that have been sent to a peer
               and have been abandoned because the peer has taken too
               long to respond to them.";
          }
          leaf req-sent-cancel-sent {
            type yang:counter32;
            description
              "The number of requests that were sent to the peer and
               explicitly cancelled by the local PCEP entity sending
               a PCNtf.";
          }
          leaf rep-rcvd-unknown {
            type yang:counter32;
            description
              "The number of responses to unknown requests
               received.  A response to an unknown request is a
               response whose RP object does not contain the
               request ID of any request that is currently
               outstanding on the session.";
          }
          description
            "The stats related to PCE as peer.";
        }
        leaf pcerr-sent {
          type yang:counter32;
          description
            "The number of PCErr messages sent.";
        }
        leaf pcerr-rcvd {
          type yang:counter32;
          description
            "The number of PCErr messages received.";
        }
        leaf pcntf-sent {
          type yang:counter32;
          description
            "The number of PCNtf messages sent.";
        }
        leaf pcntf-rcvd {
          type yang:counter32;
          description
            "The number of PCNtf messages received.";
        }
        leaf keepalive-sent {
          type yang:counter32;
          description
            "The number of Keepalive messages sent.";
        }
        leaf keepalive-rcvd {
          type yang:counter32;
          description
            "The number of Keepalive messages received.";
        }
        leaf unknown-rcvd {
          type yang:counter32;
          description
            "The number of unknown messages received.";
        }
        leaf corrupt-rcvd {
          type yang:counter32;
          description
            "The number of corrupted PCEP messages received.";
        }
        container pcc {
          when "../../pcep:role = 'pcc'"
             + "or "
             + "../../pcep:role = 'pcc-and-pce'" {
            description
              "Valid for PCEP peer as PCC.";
          }
          leaf req-rcvd {
            type yang:counter32;
            description
              "The number of requests received.  A request
               corresponds 1:1 with an RP object in a PCReq
               message.
               This might be greater than pcreq-rcvd because
               multiple requests can be batched into a single
               PCReq message.";
          }
          leaf req-rcvd-pend-rep {
            type yang:counter32;
            description
              "The number of requests that have been received for
               which a response is still pending.";
          }
          leaf req-rcvd-ero-sent {
            type yang:counter32;
            description
              "The number of requests that have been received for
               which a response with an ERO object was sent.  Such
               responses indicate that a path was successfully
               computed by the local PCEP entity.";
          }
          leaf req-rcvd-nopath-sent {
            type yang:counter32;
            description
              "The number of requests that have been received for
               which a response with a NO-PATH object was sent.  Such
               responses indicate that the local PCEP entity could
               not find a path to satisfy the request.";
          }
          leaf req-rcvd-cancel-sent {
            type yang:counter32;
            description
              "The number of requests received that were cancelled
               by the local PCEP entity sending a PCNtf message.
               This might be different than pcntf-sent because
               not all PCNtf messages are used to cancel requests,
               and a single PCNtf message can cancel multiple
               requests.";
          }
          leaf req-rcvd-error-sent {
            type yang:counter32;
            description
              "The number of requests received that were cancelled
               by the local PCEP entity sending a PCErr message.
               This might be different than pcerr-sent because
               not all PCErr messages are used to cancel requests,
               and a single PCErr message can cancel multiple
               requests.";
          }
          leaf req-rcvd-cancel-rcvd {
            type yang:counter32;
            description
              "The number of requests that were received from the
               peer and explicitly cancelled by the peer sending
               a PCNtf.";
          }
          leaf req-rcvd-unknown {
            type yang:counter32;
            description
              "The number of unknown requests that have been
               received.  An unknown request is a request
               whose RP object contains a request ID of zero.";
          }
          description
            "The stats related to PCC as peer.";
        }
        container svec {
          if-feature "pcep:svec";
          description
            "If synchronized path computation is supported.";
          container pce {
            when "../../../pcep:role = 'pce'"
               + "or "
               + "../../../pcep:role = 'pcc-and-pce'" {
              description
                "Valid for PCEP peer as PCE.";
            }
            leaf svec-sent {
              type yang:counter32;
              description
                "The number of SVEC objects sent in PCReq messages.
                 An SVEC object represents a set of synchronized
                 requests.";
            }
            leaf svec-req-sent {
              type yang:counter32;
              description
                "The number of requests sent that appeared in one
                 or more SVEC objects.";
            }
            description
              "The SVEC stats related to PCE.";
          }
          container pcc {
            when "../../../pcep:role = 'pcc'"
               + "or "
               + "../../../pcep:role = 'pcc-and-pce'" {
              description
                "Valid for PCEP peer as PCC.";
            }
            leaf svec-rcvd {
              type yang:counter32;
              description
                "The number of SVEC objects received in PCReq
                 messages.  An SVEC object represents a set of
                 synchronized requests.";
            }
            leaf svec-req-rcvd {
              type yang:counter32;
              description
                "The number of requests received that appeared
                 in one or more SVEC objects.";
            }
            description
              "The SVEC stats related to PCC as peer.";
          }
        }
        container stateful {
          if-feature "pcep:stateful";
          description
            "Stateful PCE-related statistics.";
          container pce {
            when "../../../pcep:role = 'pce'"
               + "or "
               + "../../../pcep:role = 'pcc-and-pce'" {
              description
                "Valid for PCEP peer as PCE.";
            }
            leaf pcrpt-sent {
              type yang:counter32;
              description
                "The number of PCRpt messages sent.";
            }
            leaf pcupd-rcvd {
              type yang:counter32;
              description
                "The number of PCUpd messages received.";
            }
            leaf rpt-sent {
              type yang:counter32;
              description
                "The number of LSP reports sent.  An LSP report
                 corresponds 1:1 with an LSP object in a PCRpt
                 message.  This might be greater than
                 pcrpt-sent because multiple reports can
                 be batched into a single PCRpt message.";
            }
            leaf upd-rcvd {
              type yang:counter32;
              description
                "The number of LSP updates received.  An LSP update
                 corresponds 1:1 with an LSP object in a PCUpd
                 message.
                 This might be greater than pcupd-rcvd because
                 multiple updates can be batched into a single
                 PCUpd message.";
            }
            leaf upd-rcvd-unknown {
              type yang:counter32;
              description
                "The number of updates to unknown LSPs
                 received.  An update to an unknown LSP is a
                 update whose LSP object does not contain the
                 PLSP-ID of any LSP that is currently
                 present.";
            }
            leaf upd-rcvd-undelegated {
              type yang:counter32;
              description
                "The number of updates to not delegated LSPs
                 received.  An update to an undelegated LSP is a
                 update whose LSP object does not contain the
                 PLSP-ID of any LSP that is currently
                 delegated to the current PCEP session.";
            }
            leaf upd-rcvd-error-sent {
              type yang:counter32;
              description
                "The number of updates to LSPs received that were
                 responded by the local PCEP entity by sending a
                 PCErr message.";
            }
            description
              "The stateful stats related to PCE as peer";
          }
          container pcc {
            when "../../../pcep:role = 'pcc'"
               + "or "
               + "../../../pcep:role = 'pcc-and-pce'" {
              description
                "Valid for PCEP peer as PCC.";
            }
            leaf pcrpt-rcvd {
              type yang:counter32;
              description
                "The number of PCRpt messages received.";
            }
            leaf pcupd-sent {
              type yang:counter32;
              description
                "The number of PCUpd messages sent.";
            }
            leaf rpt-rcvd {
              type yang:counter32;
              description
                "The number of LSP reports received.  An LSP report
                 corresponds 1:1 with an LSP object in a PCRpt
                 message.
                 This might be greater than pcrpt-rcvd because
                 multiple reports can be batched into a single
                 PCRpt message.";
            }
            leaf rpt-rcvd-error-sent {
              type yang:counter32;
              description
                "The number of reports of LSPs received that were
                 responded by the local PCEP entity by sending a
                 PCErr message.";
            }
            leaf upd-sent {
              type yang:counter32;
              description
                "The number of LSP updates sent.  An LSP update
                 corresponds 1:1 with an LSP object in a PCUpd
                 message.  This might be greater than
                 pcupd-sent because multiple updates can
                 be batched into a single PCUpd message.";
            }
            description
              "The stateful stats related to PCC as peer.";
          }
          container initiation {
            if-feature "pcep:pce-initiated";
            description
              "PCE-initiated related statistics.";
            container pcc {
              when "../../../../pcep:role = 'pcc'"
                 + "or "
                 + "../../../../pcep:role = 'pcc-and-pce'" {
                description
                  "Valid for PCEP peer as PCC.";
              }
              leaf pcinitiate-sent {
                type yang:counter32;
                description
                  "The number of PCInitiate messages sent.";
              }
              leaf initiate-sent {
                type yang:counter32;
                description
                  "The number of LSP initiations sent via PCE.
                   An LSP initiation corresponds 1:1 with an LSP
                   object in a PCInitiate message.  This might be
                   greater than pcinitiate-sent because
                   multiple initiations can be batched into a
                   single PCInitiate message.";
              }
              description
                "The initiation stats related to PCC as peer.";
            }
            container pce {
              when "../../../../pcep:role = 'pce'"
                 + "or "
                 + "../../../../pcep:role = 'pcc-and-pce'" {
                description
                  "Valid for PCEP peer as PCE.";
              }
              leaf pcinitiate-rcvd {
                type yang:counter32;
                description
                  "The number of PCInitiate messages received.";
              }
              leaf initiate-rcvd {
                type yang:counter32;
                description
                  "The number of LSP initiations received from
                   PCE.  An LSP initiation corresponds 1:1 with
                   an LSP object in a PCInitiate message.  This
                   might be greater than pcinitiate-rcvd
                   because multiple initiations can be batched
                   into a single PCInitiate message.";
              }
              leaf initiate-rcvd-error-sent {
                type yang:counter32;
                description
                  "The number of initiations of LSPs received
                   that were responded to by the local PCEP entity
                   by sending a PCErr message.";
              }
              description
                "The initiation stats related to PCE as peer.";
            }
          }
        }
        container path-key {
          when "../../pcep:role = 'pcc'"
             + "or "
             + "../../pcep:role = 'pcc-and-pce'" {
            description
              "Valid for PCEP peer as PCC.";
          }
          if-feature "pcep:path-key";
          description
            "If path-key is supported.";
          leaf unknown-path-key {
            type yang:counter32;
            description
              "The number of attempts to expand an unknown
               path-key.";
          }
          leaf exp-path-key {
            type yang:counter32;
            description
              "The number of attempts to expand an expired
               path-key.";
          }
          leaf dup-path-key {
            type yang:counter32;
            description
              "The number of duplicate attempts to expand the same
               path-key.";
          }
          leaf path-key-no-attempt {
            type yang:counter32;
            description
              "The number of expired path-keys with no attempt to
               expand it.";
          }
        }
        action reset-statistics {
          description
            "The reset action will clear the statistics at the
             associated container.";
          input {
            leaf reset-at {
              type yang:date-and-time;
              description
                "The time when the reset was issued.";
            }
          }
          output {
            leaf reset-finished-at {
              type yang:date-and-time;
              description
                "The time when the reset finished.";
            }
          }
        }
      }

      /*
       * Augment modules to add statistics
       */

      augment "/pcep:pcep/pcep:entity/pcep:peers/pcep:peer" {
        description
          "Augmenting the statistics.";
        container stats {
          config false;
          description
            "The container for all statistics at peer level.";
          uses stats {
            description
              "Since PCEP sessions can be ephemeral, the peer statistics
               tracks a peer even when no PCEP session currently exists
               to that peer.  The statistics contained are an aggregate
               of the statistics for all successive sessions to that
               peer.";
          }
          leaf sess-setup-ok {
            type yang:counter32;
            config false;
            description
              "The number of PCEP sessions successfully established with
               the peer, including any current session.  This counter is
               incremented each time a session with this peer is
               successfully established.";
          }
          leaf sess-setup-fail {
            type yang:counter32;
            config false;
            description
              "The number of PCEP sessions with the peer
               that have been attempted but failed
               before being fully established.  This
               counter is incremented each time a
               session retry to this peer fails.";
          }
          leaf req-sent-closed {
            when "../../pcep:role = 'pce'"
               + "or "
               + "../../pcep:role = 'pcc-and-pce'" {
              description
                "Valid for PCEP peer as PCE.";
            }
            type yang:counter32;
            description
              "The number of requests that were sent to the peer and
               implicitly cancelled when the session they were sent
               over was closed.";
          }
          leaf req-rcvd-closed {
            when "../../pcep:role = 'pcc'"
               + "or "
               + "../../pcep:role = 'pcc-and-pce'" {
              description
                "Valid for PCEP peer as PCC.";
            }
            type yang:counter32;
            description
              "The number of requests that were received from the peer
               and implicitly cancelled when the session they were
               received over was closed.";
          }
        }
      }

      augment "/pcep:pcep/pcep:entity/pcep:peers/pcep:peer/"
            + "pcep:sessions/pcep:session" {
        description
          "Augmenting the statistics.";
        container stats {
          description
            "The container for all statistics at session level.";
          uses stats {
            description
              "The statistics contained are for the current sessions to
               that peer.  These are lost when the session goes down.";
          }
        }
      }

      rpc reset-pcep-statistics-all {
        if-feature "reset-all";
        description
          "Reset all the PCEP statistics collected across all peers
           and sessions.  This RPC is used if the implementation
           supports a mechanism to reset all PCEP statistics across
           all peers and sessions through mechanisms such as by
           walking a list of pointers to those peers and sessions.

           If this mechanism is not supported, implementations must
           reset PCEP statistics individually by invoking the action
           for each peer and session.";
      }
    }

    <CODE ENDS>

¶

## 9. Security Considerations

This section is modeled after the template described in Section 3.7.1 of [YANG-GUIDELINES].¶

The "ietf-pcep" and "ietf-pcep-stats" YANG modules define data models that are designed to be accessed via YANG-based management protocols, such as NETCONF [RFC6241] and RESTCONF [RFC8040]. These protocols have to use a secure transport layer (e.g., SSH [RFC4252], TLS [RFC8446], and QUIC [RFC9000]) and have to use mutual authentication.¶

The Network Configuration Access Control Model (NACM) [RFC8341] provides the means to restrict access for particular NETCONF or RESTCONF users to a preconfigured subset of all available NETCONF or RESTCONF protocol operations and content.¶

The "ietf-pcep" YANG module:¶

There are a number of data nodes defined in the "ietf-pcep" YANG module that are writable/creatable/deletable (i.e., "config true", which is the default). All writable data nodes are likely to be reasonably sensitive or vulnerable in some network environments. Write operations (e.g., edit-config) and delete operations to these data nodes without proper protection or authentication can have a negative effect on network operations. The following subtrees and data nodes have particular sensitivities/vulnerabilities:¶

- /pcep/entity/: Configures local parameters, capabilities, etc.¶
- /pcep/entity/peers: Configures remote peers to set up a PCEP session.¶

Unauthorized access to the above list can adversely affect the PCEP session between the local entity and the peers. This may lead to the inability to compute new paths, and stateful operations on the delegated as well as PCE-initiated LSPs.¶

Some of the readable data nodes in this YANG module may be considered sensitive or vulnerable in some network environments. It is thus important to control read access (e.g., via get, get-config, or notification) to these data nodes. Specifically, the following subtrees and data nodes have particular sensitivities/ vulnerabilities:¶

- /pcep/lsp-db: All the LSPs in the network. Unauthorized access to this could provide all path and network usage information.¶
- /pcep/path-keys/: The Confidential Path Segments (CPS) are hidden using path-keys. Unauthorized access to this could leak confidential path information.¶

Some of the RPC or action operations in this YANG module may be considered sensitive or vulnerable in some network environments. It is thus important to control access to these operations. Specifically, the following operation has particular sensitivities/ vulnerabilities:¶

- trigger-resync: Triggers resynchronization with the PCE. Unauthorized access to this could force a PCEP session into continuous state synchronization.¶

This YANG module uses groupings from other YANG modules that define nodes that may be considered sensitive or vulnerable in network environments. Refer to the Security Considerations of [RFC9645] and [RFC8776] for information as to which nodes may be considered sensitive or vulnerable in network environments.¶

The actual authentication key data (whether locally specified or part of a key-chain) is sensitive and needs to be kept secret from unauthorized parties; compromise of the key data would allow an attacker to forge PCEP traffic that would be accepted as authentic, potentially compromising the TE domain.¶

The model describes several notifications; implementations must rate-limit the generation of these notifications to avoid creating a significant notification load. Otherwise, this notification load may have some side effects on the system stability and may be exploited as an attack vector.¶

The "auth" container includes various authentication and security options for PCEP. Further, Section 7.1 describes how to configure TLS 1.2 and TLS 1.3 for a PCEP session via this YANG module.¶

The "ietf-pcep-stats" YANG module:¶

There are no particularly sensitive writable data nodes.¶

There are no particularly sensitive readable data nodes.¶

Some of the RPC or action operations in this YANG module may be considered sensitive or vulnerable in some network environments. It is thus important to control access to these operations. Specifically, the following operation has particular sensitivities/vulnerabilities:¶

- reset-pcep-statistics-all: The RPC is used to reset all PCEP statistics across all peers and sessions. An unauthorized reset could impact monitoring.¶

## 10. IANA Considerations

IANA has registered the following URIs in the "IETF XML Registry" [RFC3688]:¶

URI:
  urn:ietf:params:xml:ns:yang:ietf-pcep¶
Registrant Contact:
  The IESG¶
XML:
  N/A; the requested URI is an XML namespace.¶

URI:
  urn:ietf:params:xml:ns:yang:ietf-pcep-stats¶
Registrant Contact:
  The IESG¶
XML:
  N/A; the requested URI is an XML namespace.¶

IANA has registered the following YANG modules in the "YANG Module Names" registry [RFC6020]:¶

Name:
  ietf-pcep¶
Namespace:
  urn:ietf:params:xml:ns:yang:ietf-pcep¶
Prefix:
  pcep¶
Reference:
  RFC 9826¶

Name:
  ietf-pcep-stats¶
Namespace:
  urn:ietf:params:xml:ns:yang:ietf-pcep-stats¶
Prefix:
  pcep-stats¶
Reference:
  RFC 9826¶

## 11. References

### 11.1. Normative References

[RFC2119]
  Bradner, S., "Key words for use in RFCs to Indicate Requirement Levels", BCP 14, RFC 2119, DOI 10.17487/RFC2119, March 1997, <https://www.rfc-editor.org/info/rfc2119>.
[RFC3688]
  Mealling, M., "The IETF XML Registry", BCP 81, RFC 3688, DOI 10.17487/RFC3688, January 2004, <https://www.rfc-editor.org/info/rfc3688>.
[RFC4252]
  Ylonen, T. and C. Lonvick, Ed., "The Secure Shell (SSH) Authentication Protocol", RFC 4252, DOI 10.17487/RFC4252, January 2006, <https://www.rfc-editor.org/info/rfc4252>.
[RFC5088]
  Le Roux, JL., Ed., Vasseur, JP., Ed., Ikejiri, Y., and R. Zhang, "OSPF Protocol Extensions for Path Computation Element (PCE) Discovery", RFC 5088, DOI 10.17487/RFC5088, January 2008, <https://www.rfc-editor.org/info/rfc5088>.
[RFC5089]
  Le Roux, JL., Ed., Vasseur, JP., Ed., Ikejiri, Y., and R. Zhang, "IS-IS Protocol Extensions for Path Computation Element (PCE) Discovery", RFC 5089, DOI 10.17487/RFC5089, January 2008, <https://www.rfc-editor.org/info/rfc5089>.
[RFC5440]
  Vasseur, JP., Ed. and JL. Le Roux, Ed., "Path Computation Element (PCE) Communication Protocol (PCEP)", RFC 5440, DOI 10.17487/RFC5440, March 2009, <https://www.rfc-editor.org/info/rfc5440>.
[RFC5520]
  Bradford, R., Ed., Vasseur, JP., and A. Farrel, "Preserving Topology Confidentiality in Inter-Domain Path Computation Using a Path-Key-Based Mechanism", RFC 5520, DOI 10.17487/RFC5520, April 2009, <https://www.rfc-editor.org/info/rfc5520>.
[RFC5541]
  Le Roux, JL., Vasseur, JP., and Y. Lee, "Encoding of Objective Functions in the Path Computation Element Communication Protocol (PCEP)", RFC 5541, DOI 10.17487/RFC5541, June 2009, <https://www.rfc-editor.org/info/rfc5541>.
[RFC5557]
  Lee, Y., Le Roux, JL., King, D., and E. Oki, "Path Computation Element Communication Protocol (PCEP) Requirements and Protocol Extensions in Support of Global Concurrent Optimization", RFC 5557, DOI 10.17487/RFC5557, July 2009, <https://www.rfc-editor.org/info/rfc5557>.
[RFC5925]
  Touch, J., Mankin, A., and R. Bonica, "The TCP Authentication Option", RFC 5925, DOI 10.17487/RFC5925, June 2010, <https://www.rfc-editor.org/info/rfc5925>.
[RFC6020]
  Bjorklund, M., Ed., "YANG - A Data Modeling Language for the Network Configuration Protocol (NETCONF)", RFC 6020, DOI 10.17487/RFC6020, October 2010, <https://www.rfc-editor.org/info/rfc6020>.
[RFC6241]
  Enns, R., Ed., Bjorklund, M., Ed., Schoenwaelder, J., Ed., and A. Bierman, Ed., "Network Configuration Protocol (NETCONF)", RFC 6241, DOI 10.17487/RFC6241, June 2011, <https://www.rfc-editor.org/info/rfc6241>.
[RFC6991]
  Schoenwaelder, J., Ed., "Common YANG Data Types", RFC 6991, DOI 10.17487/RFC6991, July 2013, <https://www.rfc-editor.org/info/rfc6991>.
[RFC7950]
  Bjorklund, M., Ed., "The YANG 1.1 Data Modeling Language", RFC 7950, DOI 10.17487/RFC7950, August 2016, <https://www.rfc-editor.org/info/rfc7950>.
[RFC8040]
  Bierman, A., Bjorklund, M., and K. Watsen, "RESTCONF Protocol", RFC 8040, DOI 10.17487/RFC8040, January 2017, <https://www.rfc-editor.org/info/rfc8040>.
[RFC8174]
  Leiba, B., "Ambiguity of Uppercase vs Lowercase in RFC 2119 Key Words", BCP 14, RFC 8174, DOI 10.17487/RFC8174, May 2017, <https://www.rfc-editor.org/info/rfc8174>.
[RFC8177]
  Lindem, A., Ed., Qu, Y., Yeung, D., Chen, I., and J. Zhang, "YANG Data Model for Key Chains", RFC 8177, DOI 10.17487/RFC8177, June 2017, <https://www.rfc-editor.org/info/rfc8177>.
[RFC8231]
  Crabbe, E., Minei, I., Medved, J., and R. Varga, "Path Computation Element Communication Protocol (PCEP) Extensions for Stateful PCE", RFC 8231, DOI 10.17487/RFC8231, September 2017, <https://www.rfc-editor.org/info/rfc8231>.
[RFC8232]
  Crabbe, E., Minei, I., Medved, J., Varga, R., Zhang, X., and D. Dhody, "Optimizations of Label Switched Path State Synchronization Procedures for a Stateful PCE", RFC 8232, DOI 10.17487/RFC8232, September 2017, <https://www.rfc-editor.org/info/rfc8232>.
[RFC8253]
  Lopez, D., Gonzalez de Dios, O., Wu, Q., and D. Dhody, "PCEPS: Usage of TLS to Provide a Secure Transport for the Path Computation Element Communication Protocol (PCEP)", RFC 8253, DOI 10.17487/RFC8253, October 2017, <https://www.rfc-editor.org/info/rfc8253>.
[RFC8281]
  Crabbe, E., Minei, I., Sivabalan, S., and R. Varga, "Path Computation Element Communication Protocol (PCEP) Extensions for PCE-Initiated LSP Setup in a Stateful PCE Model", RFC 8281, DOI 10.17487/RFC8281, December 2017, <https://www.rfc-editor.org/info/rfc8281>.
[RFC8282]
  Oki, E., Takeda, T., Farrel, A., and F. Zhang, "Extensions to the Path Computation Element Communication Protocol (PCEP) for Inter-Layer MPLS and GMPLS Traffic Engineering", RFC 8282, DOI 10.17487/RFC8282, December 2017, <https://www.rfc-editor.org/info/rfc8282>.
[RFC8306]
  Zhao, Q., Dhody, D., Ed., Palleti, R., and D. King, "Extensions to the Path Computation Element Communication Protocol (PCEP) for Point-to-Multipoint Traffic Engineering Label Switched Paths", RFC 8306, DOI 10.17487/RFC8306, November 2017, <https://www.rfc-editor.org/info/rfc8306>.
[RFC8340]
  Bjorklund, M. and L. Berger, Ed., "YANG Tree Diagrams", BCP 215, RFC 8340, DOI 10.17487/RFC8340, March 2018, <https://www.rfc-editor.org/info/rfc8340>.
[RFC8341]
  Bierman, A. and M. Bjorklund, "Network Configuration Access Control Model", STD 91, RFC 8341, DOI 10.17487/RFC8341, March 2018, <https://www.rfc-editor.org/info/rfc8341>.
[RFC8408]
  Sivabalan, S., Tantsura, J., Minei, I., Varga, R., and J. Hardwick, "Conveying Path Setup Type in PCE Communication Protocol (PCEP) Messages", RFC 8408, DOI 10.17487/RFC8408, July 2018, <https://www.rfc-editor.org/info/rfc8408>.
[RFC8446]
  Rescorla, E., "The Transport Layer Security (TLS) Protocol Version 1.3", RFC 8446, DOI 10.17487/RFC8446, August 2018, <https://www.rfc-editor.org/info/rfc8446>.
[RFC8623]
  Palle, U., Dhody, D., Tanaka, Y., and V. Beeram, "Stateful Path Computation Element (PCE) Protocol Extensions for Usage with Point-to-Multipoint TE Label Switched Paths (LSPs)", RFC 8623, DOI 10.17487/RFC8623, June 2019, <https://www.rfc-editor.org/info/rfc8623>.
[RFC8664]
  Sivabalan, S., Filsfils, C., Tantsura, J., Henderickx, W., and J. Hardwick, "Path Computation Element Communication Protocol (PCEP) Extensions for Segment Routing", RFC 8664, DOI 10.17487/RFC8664, December 2019, <https://www.rfc-editor.org/info/rfc8664>.
[RFC8685]
  Zhang, F., Zhao, Q., Gonzalez de Dios, O., Casellas, R., and D. King, "Path Computation Element Communication Protocol (PCEP) Extensions for the Hierarchical Path Computation Element (H-PCE) Architecture", RFC 8685, DOI 10.17487/RFC8685, December 2019, <https://www.rfc-editor.org/info/rfc8685>.
[RFC8697]
  Minei, I., Crabbe, E., Sivabalan, S., Ananthakrishnan, H., Dhody, D., and Y. Tanaka, "Path Computation Element Communication Protocol (PCEP) Extensions for Establishing Relationships between Sets of Label Switched Paths (LSPs)", RFC 8697, DOI 10.17487/RFC8697, January 2020, <https://www.rfc-editor.org/info/rfc8697>.
[RFC8745]
  Ananthakrishnan, H., Sivabalan, S., Barth, C., Minei, I., and M. Negi, "Path Computation Element Communication Protocol (PCEP) Extensions for Associating Working and Protection Label Switched Paths (LSPs) with Stateful PCE", RFC 8745, DOI 10.17487/RFC8745, March 2020, <https://www.rfc-editor.org/info/rfc8745>.
[RFC8776]
  Saad, T., Gandhi, R., Liu, X., Beeram, V., and I. Bryskin, "Common YANG Data Types for Traffic Engineering", RFC 8776, DOI 10.17487/RFC8776, June 2020, <https://www.rfc-editor.org/info/rfc8776>.
[RFC8779]
  Margaria, C., Ed., Gonzalez de Dios, O., Ed., and F. Zhang, Ed., "Path Computation Element Communication Protocol (PCEP) Extensions for GMPLS", RFC 8779, DOI 10.17487/RFC8779, July 2020, <https://www.rfc-editor.org/info/rfc8779>.
[RFC8800]
  Litkowski, S., Sivabalan, S., Barth, C., and M. Negi, "Path Computation Element Communication Protocol (PCEP) Extension for Label Switched Path (LSP) Diversity Constraint Signaling", RFC 8800, DOI 10.17487/RFC8800, July 2020, <https://www.rfc-editor.org/info/rfc8800>.
[RFC9000]
  Iyengar, J., Ed. and M. Thomson, Ed., "QUIC: A UDP-Based Multiplexed and Secure Transport", RFC 9000, DOI 10.17487/RFC9000, May 2021, <https://www.rfc-editor.org/info/rfc9000>.
[RFC9005]
  Litkowski, S., Sivabalan, S., Tantsura, J., Hardwick, J., and C. Li, "Path Computation Element Communication Protocol (PCEP) Extension for Associating Policies and Label Switched Paths (LSPs)", RFC 9005, DOI 10.17487/RFC9005, March 2021, <https://www.rfc-editor.org/info/rfc9005>.
[RFC9129]
  Yeung, D., Qu, Y., Zhang, Z., Chen, I., and A. Lindem, "YANG Data Model for the OSPF Protocol", RFC 9129, DOI 10.17487/RFC9129, October 2022, <https://www.rfc-editor.org/info/rfc9129>.
[RFC9130]
  Litkowski, S., Ed., Yeung, D., Lindem, A., Zhang, J., and L. Lhotka, "YANG Data Model for the IS-IS Protocol", RFC 9130, DOI 10.17487/RFC9130, October 2022, <https://www.rfc-editor.org/info/rfc9130>.
[RFC9168]
  Dhody, D., Farrel, A., and Z. Li, "Path Computation Element Communication Protocol (PCEP) Extension for Flow Specification", RFC 9168, DOI 10.17487/RFC9168, January 2022, <https://www.rfc-editor.org/info/rfc9168>.
[RFC9353]
  Lopez, D., Wu, Q., Dhody, D., Ma, Q., and D. King, "IGP Extension for Path Computation Element Communication Protocol (PCEP) Security Capability Support in PCE Discovery (PCED)", RFC 9353, DOI 10.17487/RFC9353, January 2023, <https://www.rfc-editor.org/info/rfc9353>.
[RFC9358]
  Lee, Y., Zheng, H., and D. Ceccarelli, "Path Computation Element Communication Protocol (PCEP) Extensions for Establishing Relationships between Sets of Label Switched Paths and Virtual Networks", RFC 9358, DOI 10.17487/RFC9358, February 2023, <https://www.rfc-editor.org/info/rfc9358>.
[RFC9645]
  Watsen, K., "YANG Groupings for TLS Clients and TLS Servers", RFC 9645, DOI 10.17487/RFC9645, October 2024, <https://www.rfc-editor.org/info/rfc9645>.

### 11.2. Informative References

[IANA-IGP]
  IANA, "Path Computation Element (PCE) Capability Flags", <https://www.iana.org/assignments/igp-parameters>.
[IANA-PCEP]
  IANA, "ASSOCIATION Type Field", <https://www.iana.org/assignments/pcep>.
[PCEPS-UPDATE]
  Dhody, D., Turner, S., and R. Housley, "Updates for PCEPS: TLS Connection Establishment Restrictions", Work in Progress, Internet-Draft, draft-ietf-pce-pceps-tls13-04, 9 January 2024, <https://datatracker.ietf.org/doc/html/draft-ietf-pce-pceps-tls13-04>.
[RFC4655]
  Farrel, A., Vasseur, J.-P., and J. Ash, "A Path Computation Element (PCE)-Based Architecture", RFC 4655, DOI 10.17487/RFC4655, August 2006, <https://www.rfc-editor.org/info/rfc4655>.
[RFC5246]
  Dierks, T. and E. Rescorla, "The Transport Layer Security (TLS) Protocol Version 1.2", RFC 5246, DOI 10.17487/RFC5246, August 2008, <https://www.rfc-editor.org/info/rfc5246>.
[RFC7420]
  Koushik, A., Stephan, E., Zhao, Q., King, D., and J. Hardwick, "Path Computation Element Communication Protocol (PCEP) Management Information Base (MIB) Module", RFC 7420, DOI 10.17487/RFC7420, December 2014, <https://www.rfc-editor.org/info/rfc7420>.
[RFC8051]
  Zhang, X., Ed. and I. Minei, Ed., "Applicability of a Stateful Path Computation Element (PCE)", RFC 8051, DOI 10.17487/RFC8051, January 2017, <https://www.rfc-editor.org/info/rfc8051>.
[RFC8342]
  Bjorklund, M., Schoenwaelder, J., Shafer, P., Watsen, K., and R. Wilton, "Network Management Datastore Architecture (NMDA)", RFC 8342, DOI 10.17487/RFC8342, March 2018, <https://www.rfc-editor.org/info/rfc8342>.
[RFC8751]
  Dhody, D., Lee, Y., Ceccarelli, D., Shin, J., and D. King, "Hierarchical Stateful Path Computation Element (PCE)", RFC 8751, DOI 10.17487/RFC8751, March 2020, <https://www.rfc-editor.org/info/rfc8751>.
[RFC9603]
  Li, C., Ed., Kaladharan, P., Sivabalan, S., Koldychev, M., and Y. Zhu, "Path Computation Element Communication Protocol (PCEP) Extensions for IPv6 Segment Routing", RFC 9603, DOI 10.17487/RFC9603, July 2024, <https://www.rfc-editor.org/info/rfc9603>.
[YANG-GUIDELINES]
  Bierman, A., Boucadair, M., and Q. Wu, "Guidelines for Authors and Reviewers of Documents Containing YANG Data Models", Work in Progress, Internet-Draft, draft-ietf-netmod-rfc8407bis-28, 5 June 2025, <https://datatracker.ietf.org/doc/html/draft-ietf-netmod-rfc8407bis-28>.
[YANG-PCEP-SRV6]
  Li, C., Sivabalan, S., Peng, S., Koldychev, M., and L. Ndifor, "A YANG Data Model for Segment Routing (SR) Policy and SR in IPv6 (SRv6) support in Path Computation Element Communications Protocol (PCEP)", Work in Progress, Internet-Draft, draft-ietf-pce-pcep-srv6-yang-07, 21 April 2025, <https://datatracker.ietf.org/doc/html/draft-ietf-pce-pcep-srv6-yang-07>.
[YANG-TE]
  Saad, T., Gandhi, R., Liu, X., Beeram, V. P., and I. Bryskin, "A YANG Data Model for Traffic Engineering Tunnels, Label Switched Paths and Interfaces", Work in Progress, Internet-Draft, draft-ietf-teas-yang-te-38, 29 May 2025, <https://datatracker.ietf.org/doc/html/draft-ietf-teas-yang-te-38>.

## Appendix A. The Full PCEP Data Model

The module "ietf-pcep" defines the basic components of a PCE speaker. The tree depth in the tree is set to 10.¶

    module: ietf-pcep
      +--rw pcep!
         +--rw entity
            +--rw addr*                         inet:ip-address-no-zone
            +--rw enabled?                      boolean
            +--rw role                          role
            +--rw description?                  string
            +--rw speaker-entity-id?            string {sync-opt}?
            +--rw admin-status?                 boolean
            +--ro index?                        uint32
            +--ro oper-status?                  oper-status
            +--rw domains
            |  +--rw domain* [type domain]
            |     +--rw type      identityref
            |     +--rw domain    domain
            +--rw capabilities
            |  +--rw capability?             bits
            |  +--rw pce-initiated?          boolean {pce-initiated}?
            |  +--rw include-db-ver?         boolean {stateful,sync-opt}?
            |  +--rw trigger-resync?         boolean {stateful,sync-opt}?
            |  +--rw trigger-initial-sync?   boolean {stateful,sync-opt}?
            |  +--rw incremental-sync?       boolean {stateful,sync-opt}?
            |  +--rw sr-mpls {sr-mpls}?
            |  |  +--rw enabled?        boolean
            |  |  +--rw no-msd-limit?   boolean
            |  |  +--rw nai?            boolean
            |  +--rw stateful-gmpls {stateful,gmpls}?
            |  |  +--rw enabled?   boolean
            |  +--rw inter-layer?            boolean {inter-layer}?
            |  +--rw h-pce {h-pce}?
            |     +--rw enabled?    boolean
            |     +--rw stateful?   boolean {stateful}?
            |     +--rw role?       hpce-role
            +--ro msd?                          uint8 {sr-mpls}?
            +--rw auth
            |  +--rw (auth-type-selection)?
            |     +--:(auth-key-chain)
            |     |  +--rw key-chain?
            |     |          key-chain:key-chain-ref
            |     +--:(auth-key)
            |     |  +--rw crypto-algorithm            identityref
            |     |  +--rw (key-string-style)?
            |     |     +--:(keystring)
            |     |     |  +--rw keystring?            string
            |     |     +--:(hexadecimal) {key-chain:hex-key-string}?
            |     |        +--rw hexadecimal-string?   yang:hex-string
            |     +--:(auth-tls) {tls}?
            |        +--rw (role)?
            |           +--:(server)
            |           |  +--rw tls-server
            |           |     +--rw server-identity
            |           |     |  +--rw (auth-type)
            |           |     |        ...
            |           |     +--rw client-authentication!
            |           |     |       {client-auth-supported}?
            |           |     |  +--rw ca-certs! {client-auth-x509-cert}?
            |           |     |  |     ...
            |           |     |  +--rw ee-certs! {client-auth-x509-cert}?
            |           |     |  |     ...
            |           |     |  +--rw raw-public-keys!
            |           |     |  |       {client-auth-raw-public-key}?
            |           |     |  |     ...
            |           |     |  +--rw tls12-psks?        empty
            |           |     |  |       {client-auth-tls12-psk}?
            |           |     |  +--rw tls13-epsks?       empty
            |           |     |          {client-auth-tls13-epsk}?
            |           |     +--rw hello-params {tlscmn:hello-params}?
            |           |     |  +--rw tls-versions
            |           |     |  |     ...
            |           |     |  +--rw cipher-suites
            |           |     |        ...
            |           |     +--rw keepalives {tls-server-keepalives}?
            |           |        +--rw peer-allowed-to-send?   empty
            |           |        +--rw test-peer-aliveness!
            |           |              ...
            |           +--:(client)
            |              +--rw tls-client
            |                 +--rw client-identity!
            |                 |  +--rw (auth-type)
            |                 |        ...
            |                 +--rw server-authentication
            |                 |  +--rw ca-certs! {server-auth-x509-cert}?
            |                 |  |     ...
            |                 |  +--rw ee-certs! {server-auth-x509-cert}?
            |                 |  |     ...
            |                 |  +--rw raw-public-keys!
            |                 |  |       {server-auth-raw-public-key}?
            |                 |  |     ...
            |                 |  +--rw tls12-psks?        empty
            |                 |  |       {server-auth-tls12-psk}?
            |                 |  +--rw tls13-epsks?       empty
            |                 |          {server-auth-tls13-epsk}?
            |                 +--rw hello-params {tlscmn:hello-params}?
            |                 |  +--rw tls-versions
            |                 |  |     ...
            |                 |  +--rw cipher-suites
            |                 |        ...
            |                 +--rw keepalives {tls-client-keepalives}?
            |                    +--rw peer-allowed-to-send?   empty
            |                    +--rw test-peer-aliveness!
            |                          ...
            +--rw pce-info
            |  +--rw scope
            |  |  +--rw path-scope?         bits
            |  |  +--rw intra-area-pref?    uint8
            |  |  +--rw inter-area-pref?    uint8
            |  |  +--rw inter-as-pref?      uint8
            |  |  +--rw inter-layer-pref?   uint8
            |  +--rw neighbor-domains
            |  |  +--rw domain* [type domain]
            |  |     +--rw type      identityref
            |  |     +--rw domain    domain
            |  +--rw path-key {path-key}?
            |     +--rw enabled?         boolean
            |     +--rw discard-timer?   uint32
            |     +--rw reuse-time?      uint32
            |     +--rw pce-id?          inet:ip-address-no-zone
            +--rw connect-timer?                uint16
            +--rw connect-max-retry?            uint32
            +--rw init-back-off-timer           uint16
            +--rw max-back-off-timer            uint32
            +--ro open-wait-timer?              uint16
            +--ro keep-wait-timer?              uint16
            +--rw keepalive-timer?              uint8
            +--rw dead-timer?                   uint8
            +--rw allow-negotiation?            boolean
            +--rw max-keepalive-timer           uint8
            +--rw max-dead-timer                uint8
            +--rw min-keepalive-timer           uint8
            +--rw min-dead-timer                uint8
            +--rw sync-timer?                   uint16 {svec}?
            +--rw request-timer                 uint16
            +--rw max-sessions                  uint32
            +--rw max-unknown-reqs?             uint32
            +--rw max-unknown-msgs?             uint32
            +--rw pcep-notification-max-rate    uint32
            +--rw stateful-parameter {stateful}?
            |  +--rw state-timeout           uint32
            |  +--rw redelegation-timeout    uint32
            |  +--rw rpt-non-pcep-lsp?       boolean
            +--rw of-list {objective-function}?
            |  +--rw objective-function* [of]
            |     +--rw of    identityref
            +--ro lsp-db {stateful}?
            |  +--ro db-ver?             uint64 {sync-opt}?
            |  +--ro association-list*
            |  |       [type id source global-source extended-id]
            |  |       {association}?
            |  |  +--ro type             identityref
            |  |  +--ro id               uint16
            |  |  +--ro source           inet:ip-address-no-zone
            |  |  +--ro global-source    uint32
            |  |  +--ro extended-id      string
            |  |  +--ro lsp* [plsp-id pcc-id lsp-id]
            |  |     +--ro plsp-id    -> /pcep/entity/lsp-db/lsp/plsp-id
            |  |     +--ro pcc-id     leafref
            |  |     +--ro lsp-id     leafref
            |  +--ro lsp* [plsp-id pcc-id lsp-id]
            |     +--ro plsp-id               uint32
            |     +--ro pcc-id                inet:ip-address-no-zone
            |     +--ro source?               inet:ip-address-no-zone
            |     +--ro destination?          inet:ip-address-no-zone
            |     +--ro tunnel-id?            uint16
            |     +--ro lsp-id                uint16
            |     +--ro extended-tunnel-id?   inet:ip-address-no-zone
            |     +--ro admin-state?          boolean
            |     +--ro operational-state?    operational-state
            |     +--ro delegated
            |     |  +--ro enabled?   boolean
            |     |  +--ro peer?      -> /pcep/entity/peers/peer/addr
            |     |  +--ro srp-id?    uint32
            |     +--ro initiation {pce-initiated}?
            |     |  +--ro enabled?   boolean
            |     |  +--ro peer?      -> /pcep/entity/peers/peer/addr
            |     +--ro symbolic-path-name?   string
            |     +--ro last-error?           identityref
            |     +--ro pst?                  identityref
            |     +--ro association-list*
            |             [type id source global-source extended-id]
            |             {association}?
            |        +--ro type
            |        |       -> /pcep/entity/lsp-db/association-list/type
            |        +--ro id               leafref
            |        +--ro source           leafref
            |        +--ro global-source    leafref
            |        +--ro extended-id      leafref
            +--ro path-keys {path-key}?
            |  +--ro path-key* [key]
            |     +--ro key              uint16
            |     +--ro cps
            |     |  +--ro explicit-route-objects* [index]
            |     |     +--ro index    uint32
            |     |     +--ro (type)?
            |     |        +--:(numbered-node-hop)
            |     |        |  +--ro numbered-node-hop
            |     |        |     +--ro node-id     te-node-id
            |     |        |     +--ro hop-type?   te-hop-type
            |     |        +--:(numbered-link-hop)
            |     |        |  +--ro numbered-link-hop
            |     |        |     +--ro link-tp-id    te-tp-id
            |     |        |     +--ro hop-type?     te-hop-type
            |     |        |     +--ro direction?    te-link-direction
            |     |        +--:(unnumbered-link-hop)
            |     |        |  +--ro unnumbered-link-hop
            |     |        |     +--ro link-tp-id    te-tp-id
            |     |        |     +--ro node-id       te-node-id
            |     |        |     +--ro hop-type?     te-hop-type
            |     |        |     +--ro direction?    te-link-direction
            |     |        +--:(as-number)
            |     |        |  +--ro as-number-hop
            |     |        |     +--ro as-number    inet:as-number
            |     |        |     +--ro hop-type?    te-hop-type
            |     |        +--:(label)
            |     |           +--ro label-hop
            |     |              +--ro te-label
            |     |                    ...
            |     +--ro pcc-requester?   -> /pcep/entity/peers/peer/addr
            |     +--ro req-id?          uint32
            |     +--ro retrieved?       boolean
            |     +--ro pcc-retrieved?   -> /pcep/entity/peers/peer/addr
            |     +--ro creation-time?   yang:timestamp
            |     +--ro discard-time?    uint32
            |     +--ro reuse-time?      uint32
            +--rw peers
               +--rw peer* [addr]
                  +--rw addr                    inet:ip-address-no-zone
                  +--rw role                    role
                  +--rw description?            string
                  +--rw domains
                  |  +--rw domain* [type domain]
                  |     +--rw type      identityref
                  |     +--rw domain    domain
                  +--rw capabilities
                  |  +--rw capability?             bits
                  |  +--rw pce-initiated?          boolean
                  |  |       {pce-initiated}?
                  |  +--rw include-db-ver?         boolean
                  |  |       {stateful,sync-opt}?
                  |  +--rw trigger-resync?         boolean
                  |  |       {stateful,sync-opt}?
                  |  +--rw trigger-initial-sync?   boolean
                  |  |       {stateful,sync-opt}?
                  |  +--rw incremental-sync?       boolean
                  |  |       {stateful,sync-opt}?
                  |  +--rw sr-mpls {sr-mpls}?
                  |  |  +--rw enabled?        boolean
                  |  |  +--rw no-msd-limit?   boolean
                  |  |  +--rw nai?            boolean
                  |  +--rw stateful-gmpls {stateful,gmpls}?
                  |  |  +--rw enabled?   boolean
                  |  +--rw inter-layer?            boolean {inter-layer}?
                  |  +--rw h-pce {h-pce}?
                  |     +--rw enabled?    boolean
                  |     +--rw stateful?   boolean {stateful}?
                  |     +--rw role?       hpce-role
                  +--ro msd?                    uint8 {sr-mpls}?
                  +--rw pce-info
                  |  +--rw scope
                  |  |  +--rw path-scope?         bits
                  |  |  +--rw intra-area-pref?    uint8
                  |  |  +--rw inter-area-pref?    uint8
                  |  |  +--rw inter-as-pref?      uint8
                  |  |  +--rw inter-layer-pref?   uint8
                  |  +--rw neighbor-domains
                  |     +--rw domain* [type domain]
                  |        +--rw type      identityref
                  |        +--rw domain    domain
                  +--rw delegation-pref         uint8 {stateful}?
                  +--rw auth
                  |  +--rw (auth-type-selection)?
                  |     +--:(auth-key-chain)
                  |     |  +--rw key-chain?
                  |     |          key-chain:key-chain-ref
                  |     +--:(auth-key)
                  |     |  +--rw crypto-algorithm            identityref
                  |     |  +--rw (key-string-style)?
                  |     |     +--:(keystring)
                  |     |     |  +--rw keystring?            string
                  |     |     +--:(hexadecimal)
                  |     |              {key-chain:hex-key-string}?
                  |     |        +--rw hexadecimal-string?
                  |     |                yang:hex-string
                  |     +--:(auth-tls) {tls}?
                  |        +--rw (role)?
                  |           +--:(server)
                  |           |  +--rw tls-server
                  |           |        ...
                  |           +--:(client)
                  |              +--rw tls-client
                  |                    ...
                  +--ro discontinuity-time?     yang:timestamp
                  +--ro initiate-session?       boolean
                  +--ro session-exists?         boolean
                  +--ro session-up-time?        yang:timestamp
                  +--ro session-fail-time?      yang:timestamp
                  +--ro session-fail-up-time?   yang:timestamp
                  +--ro sessions
                     +--ro session* [initiator]
                        +--ro initiator                    initiator
                        +--ro role?
                        |       -> ../../../role
                        +--ro state-last-change?           yang:timestamp
                        +--ro state?                       sess-state
                        +--ro session-creation?            yang:timestamp
                        +--ro connect-retry?               yang:counter32
                        +--ro local-id?                    uint8
                        +--ro remote-id?                   uint8
                        +--ro keepalive-timer?             uint8
                        +--ro peer-keepalive-timer?        uint8
                        +--ro dead-timer?                  uint8
                        +--ro peer-dead-timer?             uint8
                        +--ro ka-hold-time-rem?            uint8
                        +--ro overloaded?                  boolean
                        +--ro overloaded-timestamp?        yang:timestamp
                        +--ro overload-time?               uint32
                        +--ro peer-overloaded?             boolean
                        +--ro peer-overloaded-timestamp?   yang:timestamp
                        +--ro peer-overload-time?          uint32
                        +--ro lspdb-sync?                  sync-state
                        |       {stateful}?
                        +--ro recv-db-ver?                 uint64
                        |       {stateful,sync-opt}?
                        +--ro of-list {objective-function}?
                        |  +--ro objective-function* [of]
                        |     +--ro of    identityref
                        +--ro pst-list
                        |  +--ro path-setup-type* [pst]
                        |     +--ro pst    identityref
                        +--ro assoc-type-list {association}?
                        |  +--ro assoc-type* [at]
                        |     +--ro at    identityref
                        +--ro speaker-entity-id?           string
                                {sync-opt}?

      rpcs:
        +---x trigger-resync {stateful,sync-opt}?
           +---w input
              +---w pcc    -> /pcep/entity/peers/peer/addr

      notifications:
        +---n pcep-session-up
        |  +--ro peer-addr?           -> /pcep/entity/peers/peer/addr
        |  +--ro session-initiator?   leafref
        |  +--ro state-last-change?   yang:timestamp
        |  +--ro state?               sess-state
        +---n pcep-session-down
        |  +--ro peer-addr?           -> /pcep/entity/peers/peer/addr
        |  +--ro session-initiator?   initiator
        |  +--ro state-last-change?   yang:timestamp
        |  +--ro state?               sess-state
        +---n pcep-session-local-overload
        |  +--ro peer-addr?              -> /pcep/entity/peers/peer/addr
        |  +--ro session-initiator?      leafref
        |  +--ro overloaded?             boolean
        |  +--ro overloaded-timestamp?   yang:timestamp
        |  +--ro overload-time?          uint32
        +---n pcep-session-local-overload-clear
        |  +--ro peer-addr?
        |  |       -> /pcep/entity/peers/peer/addr
        |  +--ro overloaded?                   boolean
        |  +--ro overloaded-clear-timestamp?   yang:timestamp
        +---n pcep-session-peer-overload
        |  +--ro peer-addr?
        |  |       -> /pcep/entity/peers/peer/addr
        |  +--ro session-initiator?           leafref
        |  +--ro peer-overloaded?             boolean
        |  +--ro peer-overloaded-timestamp?   yang:timestamp
        |  +--ro peer-overload-time?          uint32
        +---n pcep-session-peer-overload-clear
           +--ro peer-addr?
           |       -> /pcep/entity/peers/peer/addr
           +--ro peer-overloaded?                   boolean
           +--ro peer-overloaded-clear-timestamp?   yang:timestamp

¶

## Appendix B. Example

The example below provides an overview of PCEP peer session information and LSP-DB in the "ietf-pcep" module.¶

¶
Figure 1: Example

    at PCE:
    {
      "ietf-pcep:pcep": {
        "entity": {
          "addr": [
            "192.0.2.3",
            "2001:db8::3"
          ],
          "role": "pce",
          "oper-status": "oper-status-up",
          "capabilities": {
            "capability": "active passive"
          },
          "init-back-off-timer": 5,
          "max-back-off-timer": 3600,
          "max-keepalive-timer": 255,
          "max-dead-timer": 255,
          "min-keepalive-timer": 1,
          "min-dead-timer": 30,
          "request-timer": 300,
          "max-sessions": 2400,
          "pcep-notification-max-rate": 5,
          "stateful-parameter": {
            "state-timeout": 300
          },
          "lsp-db": {
            "lsp": [
              {
                "plsp-id": 3,
                "pcc-id": "192.0.2.1",
                "source": "192.0.2.1",
                "destination": "192.0.2.4",
                "tunnel-id": 16,
                "lsp-id": 3,
                "extended-tunnel-id": "0.0.0.0",
                "operational-state": "up",
                "delegated": {
                  "enabled": true
                },
                "symbolic-path-name": "iewauh"
              },
              {
                "plsp-id": 4,
                "pcc-id": "192.0.2.2",
                "source": "192.0.2.2",
                "destination": "192.0.2.5",
                "tunnel-id": 17,
                "lsp-id": 4,
                "extended-tunnel-id": "0.0.0.0",
                "operational-state": "up",
                "delegated": {
                  "enabled": true
                },
                "symbolic-path-name": "iewauhiewauh"
              }
            ]
          },
          "peers": {
            "peer": [
              {
                "addr": "192.0.2.1",
                "role": "pcc",
                "capabilities": {
                  "capability": "active passive"
                },
                "sessions": {
                  "session": [
                    {
                      "initiator": "remote",
                      "role": "pcc"
                    }
                  ]
                }
              },
              {
                "addr": "192.0.2.2",
                "role": "pcc",
                "capabilities": {
                  "capability": "active passive"
                },
                "sessions": {
                  "session": [
                    {
                      "initiator": "remote",
                      "role": "pcc"
                    }
                  ]
                }
              },
              {
                "addr": "2001:db8::4",
                "role": "pcc",
                "capabilities": {
                  "capability": "active passive"
                },
                "sessions": {
                  "session": [
                    {
                      "initiator": "remote",
                      "role": "pcc"
                    }
                  ]
                }
              }
            ]
          }
        }
      }
    }

¶

Similarly, a PCEP session with an IPv6 address between a PCE (2001:db8::3) and a PCC (2001:db8::4) could also be set up.¶

## Appendix C. Design Objectives

This section describes some of the design objectives for the model:¶

- Existing implementations need to map the data model defined in this document to their proprietary data model. To facilitate such mappings, the data model should be simple.¶

- The data model should be suitable for new implementations to use as is.¶

- Mapping to the PCEP MIB module [RFC7420] should be clear.¶

- The data model should allow for static configurations of peers.¶

- The data model should include read-only counters in order to gather statistics for sent and received PCEP messages, received messages with errors, and messages that could not be sent due to errors. This could be in a separate model that augments the base data model.¶

- It should be fairly straightforward to augment the base data model for advanced PCE features.¶

## Appendix D. Relationship with PCEP MIB

If a node implements the PCEP MIB [RFC7420], data nodes from the YANG module can be mapped to table entries in the PCEP MIB.¶

Table 3: High-Level Relationship with PCEP MIB
YANG Data Nodes | PCEP MIB Objects
--- | ---
/pcep/entity | PcePcepEntityEntry
/pcep/entity/peers/peer | pcePcepPeerEntry
/pcep/entity/peers/peer/sessions/session | pcePcepSessEntry

Table 4: Relationship with PCEP MIB for Entity
YANG Data Nodes | PCEP MIB Objects
--- | ---
- | pcePcepEntityIndex
admin-status | pcePcepEntityAdminStatus
oper-status | pcePcepEntityOperStatus
addr | pcePcepEntityAddrType, pcePcepEntityAddr
connect-timer | pcePcepEntityConnectTimer
connect-max-retry | pcePcepEntityConnectMaxRetry
init-back-off-timer | pcePcepEntityInitBackoffTimer
max-back-off-timer | pcePcepEntityMaxBackoffTimer
open-wait-timer | pcePcepEntityOpenWaitTimer
keep-wait-timer | pcePcepEntityKeepWaitTimer
keepalive-timer | pcePcepEntityKeepAliveTimer
dead-timer | pcePcepEntityDeadTimer
allow-negotiation | pcePcepEntityAllowNegotiation
max-keepalive-timer | pcePcepEntityMaxKeepAliveTimer
max-dead-timer | pcePcepEntityMaxDeadTimer
min-keepalive-timer | pcePcepEntityMinKeepAliveTimer
min-dead-timer | pcePcepEntityMinDeadTimer
sync-timer | pcePcepEntitySyncTimer
request-timer | pcePcepEntityRequestTimer
max-sessions | pcePcepEntityMaxSessions
max-unknown-reqs | pcePcepEntityMaxUnknownReqs
max-unknown-msgs | pcePcepEntityMaxUnknownMsgs

Table 5: Relationship with PCEP MIB for Peer
YANG Data Nodes in /pcep/entity/peers/peer | PCEP MIB Objects
--- | ---
addr | pcePcepPeerAddrType,pcePcepPeerAddr
role | pcePcepPeerRole
discontinuity-time | pcePcepPeerDiscontinuityTime
initiate-session | pcePcepPeerInitiateSession
session-exists | pcePcepPeerSessionExists
sess-setup-ok | pcePcepPeerNumSessSetupOK
sess-setup-fail | pcePcepPeerNumSessSetupFail
session-up-time | pcePcepPeerSessionUpTime
session-fail-time | pcePcepPeerSessionFailTime
session-fail-up-time | pcePcepPeerSessionFailUpTime
/stats/rsp-time-avg | pcePcepPeerAvgRspTime
/stats/rsp-time-lwm | pcePcepPeerLWMRspTime
/stats/rsp-time-hwm | pcePcepPeerHWMRspTime
/stats/pcreq-sent | pcePcepPeerNumPCReqSent
/stats/pcreq-rcvd | pcePcepPeerNumPCReqRcvd
/stats/pcrep-sent | pcePcepPeerNumPCRepSent
/stats/pcrep-rcvd | pcePcepPeerNumPCRepRcvd
/stats/pcerr-sent | pcePcepPeerNumPCErrSent
/stats/pcerr-rcvd | pcePcepPeerNumPCErrRcvd
/stats/pcntf-sent | pcePcepPeerNumPCNtfSent
/stats/pcntf-rcvd | pcePcepPeerNumPCNtfRcvd
/stats/keepalive-sent | pcePcepPeerNumKeepaliveSent
/stats/keepalive-rcvd | pcePcepPeerNumKeepaliveRcvd
/stats/unknown-rcvd | pcePcepPeerNumUnknownRcvd
/stats/corrupt-rcvd | pcePcepPeerNumCorruptRcvd
/stats/req-sent | pcePcepPeerNumReqSent
/stats/svec/svec-sent | pcePcepPeerNumSvecSent
/stats/svec/svec-req-sent | pcePcepPeerNumSvecReqSent
/stats/req-sent-pend-rep | pcePcepPeerNumReqSentPendRep
/stats/req-sent-ero-rcvd | pcePcepPeerNumReqSentEroRcvd
/stats/req-sent-nopath-rcvd | pcePcepPeerNumReqSentNoPathRcvd
/stats/req-sent-cancel-rcvd | pcePcepPeerNumReqSentCancelRcvd
/stats/req-sent-error-rcvd | pcePcepPeerNumReqSentErrorRcvd
/stats/req-sent-timeout | pcePcepPeerNumReqSentTimeout
/stats/req-sent-cancel-sent | pcePcepPeerNumReqSentCancelSent
/stats/req-sent-closed | pcePcepPeerNumReqSentClosed
/stats/req-rcvd | pcePcepPeerNumReqRcvd
/stats/svec/svec-rcvd | pcePcepPeerNumSvecRcvd
/stats/svec/svec-req-rcvd | pcePcepPeerNumSvecReqRcvd
/stats/req-rcvd-pend-rep | pcePcepPeerNumReqRcvdPendRep
/stats/req-rcvd-ero-sent | pcePcepPeerNumReqRcvdEroSent
/stats/req-rcvd-nopath-sent | pcePcepPeerNumReqRcvdNoPathSent
/stats/req-rcvd-cancel-sent | pcePcepPeerNumReqRcvdCancelSent
/stats/req-rcvd-error-sent | pcePcepPeerNumReqRcvdErrorSent
/stats/req-rcvd-cancel-rcvd | pcePcepPeerNumReqRcvdCancelRcvd
/stats/req-rcvd-closed | pcePcepPeerNumReqRcvdClosed
/stats/rep-rcvd-unknown | pcePcepPeerNumRepRcvdUnknown
/stats/req-rcvd-unknown | pcePcepPeerNumReqRcvdUnknown

Table 6: Relationship with PCEP MIB for Session
YANG Data Nodes in /pcep/entity/peers/peer/sessions/session | PCEP MIB Objects
--- | ---
initiator | pcePcepSessInitiator
state-last-change | pcePcepSessStateLastChange
state | pcePcepSessState
connect-retry | pcePcepSessConnectRetry
local-id | pcePcepSessLocalID
remote-id | pcePcepSessRemoteID
keepalive-timer | pcePcepSessKeepaliveTimer
peer-keepalive-timer | pcePcepSessPeerKeepaliveTimer
dead-timer | pcePcepSessDeadTimer
peer-dead-timer | pcePcepSessPeerDeadTimer
ka-hold-time-rem | pcePcepSessKAHoldTimeRem
overloaded | pcePcepSessOverloaded
overloaded-timestamp | pcePcepSessOverloadTime
peer-overloaded | pcePcepSessPeerOverloaded
peer-overloaded-timestamp | pcePcepSessPeerOverloadTime
/stats/discontinuity-time | pcePcepSessDiscontinuityTime
/stats/rsp-time-avg | pcePcepSessAvgRspTime
/stats/rsp-time-lwm | pcePcepSessLWMRspTime
/stats/rsp-time-hwm | pcePcepSessHWMRspTime
/stats/pcreq-sent | pcePcepSessNumPCReqSent
/stats/pcreq-rcvd | pcePcepSessNumPCReqRcvd
/stats/pcrep-sent | pcePcepSessNumPCRepSent
/stats/pcrep-rcvd | pcePcepSessNumPCRepRcvd
/stats/pcerr-sent | pcePcepSessNumPCErrSent
/stats/pcerr-rcvd | pcePcepSessNumPCErrRcvd
/stats/pcntf-sent | pcePcepSessNumPCNtfSent
/stats/pcntf-rcvd | pcePcepSessNumPCNtfRcvd
/stats/keepalive-sent | pcePcepSessNumKeepaliveSent
/stats/keepalive-rcvd | pcePcepSessNumKeepaliveRcvd
/stats/unknown-rcvd | pcePcepSessNumUnknownRcvd
/stats/corrupt-rcvd | pcePcepSessNumCorruptRcvd
/stats/req-sent | pcePcepSessNumReqSent
/stats/svec/svec-sent | pcePcepSessNumSvecSent
/stats/svec/svec-req-sent | pcePcepSessNumSvecReqSent
/stats/req-sent-pend-rep | pcePcepSessNumReqSentPendRep
/stats/req-sent-ero-rcvd | pcePcepSessNumReqSentEroRcvd
/stats/req-sent-nopath-rcvd | pcePcepSessNumReqSentNoPathRcvd
/stats/req-sent-cancel-rcvd | pcePcepSessNumReqSentCancelRcvd
/stats/req-sent-error-rcvd | pcePcepSessNumReqSentErrorRcvd
/stats/req-sent-timeout | pcePcepSessNumReqSentTimeout
/stats/req-sent-cancel-sent | pcePcepSessNumReqSentCancelSent
/stats/req-rcvd | pcePcepSessNumReqRcvd
/stats/svec/svec-rcvd | pcePcepSessNumSvecRcvd
/stats/svec/svec-req-rcvd | pcePcepSessNumSvecReqRcvd
/stats/req-rcvd-pend-rep | pcePcepSessNumReqRcvdPendRep
/stats/req-rcvd-ero-sent | pcePcepSessNumReqRcvdEroSent
/stats/req-rcvd-nopath-sent | pcePcepSessNumReqRcvdNoPathSent
/stats/req-rcvd-cancel-sent | pcePcepSessNumReqRcvdCancelSent
/stats/req-rcvd-error-sent | pcePcepSessNumReqRcvdErrorSent
/stats/req-rcvd-cancel-rcvd | pcePcepSessNumReqRcvdCancelRcvd
/stats/rep-rcvd-unknown | pcePcepSessNumRepRcvdUnknown
/stats/req-rcvd-unknown | pcePcepSessNumReqRcvdUnknown

Table 7: Relationship with PCEP MIB Notification
YANG notifications | PCEP MIB NOTIFICATIONS
--- | ---
pcep-session-up | pcePcepSessUp
pcep-session-down | pcePcepSessDown
pcep-session-local-overload | pcePcepSessLocalOverload
pcep-session-local-overload-clear | pcePcepSessLocalOverloadClear
pcep-session-peer-overload | pcePcepSessPeerOverload
pcep-session-peer-overload-clear | pcePcepSessPeerOverloadClear

## Acknowledgements

The initial draft version of this document was based on the PCEP MIB [RFC7420]. The authors of this document would like to thank the authors of [RFC7420].¶

Thanks to Martin Bjorklund and Tom Petch for the detailed review. Thanks to Mahesh Jethanandani and Jan Lindblad for the YANGDOCTOR review. Thanks to Scott Kelly for the SECDIR review. Thanks to Gyan Mishra and Matthew Bocci for the RTGDIR review.¶

## Contributors

## Authors' Addresses